{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-D / RXF-D9"]
[]
[]
[]
[]
["","","","","FTXF60D2V1B / RXF60D5V1B9","FTXF71D2V1B / RXF71D5V1B9"]
["Kühlleistung","Min.","","kW","1.7","2.3"]
["","Nom.","","kW","6","7.1"]
["","Max.","","kW","7","7.3"]
["Heizleistung","Min.","","kW","1.7","2.3"]
["","Nom.","","kW","6.4","8.2"]
["","Max.","","kW","8","9"]
["Nominale Effizienz","EER","","","3.25","2.56"]
["","COP","","","3.93","3.15"]
["","Jährlicher Energieverbrauch","","kWh","923","1387"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","A","E"]
["","","Heizen","","A","A"]
["Raumkühlen","Energieeffizienzklasse","","","A++","A"]
["","Leistung","Pdesign","kW","6","7.1"]
["","SEER","","","6.15","5.15"]
["","Jährlicher Energieverbrauch","","kWh/a","342","483"]
["Raumheizen (Durchschnittliches Klima)","Energieeffizienzklasse","","","A+","A"]
["","Leistung","Pdesign","kW","4.8","6.2"]
["","SCOP/A","","","4.06","3.81"]
["","Raumheizen (Durchschnittliches Klima)-=-Heizleistung&nbsp;Pdh bei&nbsp;-10°-=-kW","","kW","4.24","5.02"]
["","Jährlicher Energieverbrauch","","kWh/a","1654","2275"]
["Hinweise","","","","(1) - Nennkühlleistungen basieren auf: Innentemp.: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m.","(1) - Nennkühlleistungen basieren auf: Innentemp.: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m."]
["","","","","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m.","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m."]
["","","","","(3) - Siehe separate Zeichnung für den Betriebsbereich","(3) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","(4) - Siehe separate Zeichnung für die elektrischen Daten","(4) - Siehe separate Zeichnung für die elektrischen Daten"]