{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":90,"n_cols":12,"rows_kept":90,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-D"]
[]
[]
[]
[]
["","","","","","FTXF20D5V1B","FTXF25D5V1B","FTXF35D5V1B","FTXF42D5V1B","FTXF50D2V1B","FTXF60D2V1B","FTXF71D2V1B"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","","","","","0.029","","0.032"]
["","Heizen","","Nom.","kW","","","","","0.032","","0.035"]
["Gehäuse","Farbe","","","","","","","","Weiß","","Weiß"]
["Abmessungen","Gerät","","Höhe","mm","","","","","295","","295"]
["","","","Breite","mm","","","","","990","","990"]
["","","","Tiefe","mm","","","","","263","","263"]
["Gewicht","Maßeinheit","","","kg","","","","","13.5","","13.5"]
["Ventilator","Luftstromvolumen","Kühlen","Hoch","m³/min","","","","","16.8","","17.3"]
["","","","Mittel","m³/min","","","","","14.4","","14.8"]
["","","","Niedrig","m³/min","","","","","11.9","","12.2"]
["","","","Flüsterbetrieb","m³/min","","","","","10.5","","10.7"]
["","","Heizen","Hoch","m³/min","","","","","17.3","","17.9"]
["","","","Mittel","m³/min","","","","","14.8","","15.8"]
["","","","Niedrig","m³/min","","","","","12.2","","12.8"]
["","","","Flüsterbetrieb","m³/min","","","","","10.7","","11.3"]
["Schallleistungspegel","Kühlung","","","dB(A)","","","","","59","","62"]
["","Heizen","","","dB(A)","","","","","61","","62"]
["Schalldruckpegel","Kühlung","","Hoch","dB(A)","","","","","43","","46"]
["","","","Mittel","dB(A)","","","","","39","","42"]
["","","","Niedrig","dB(A)","","","","","34","","37"]
["","","","Flüsterbetrieb","dB(A)","","","","","31","","34"]
["","Heizen","","Hoch","dB(A)","","","","","42","","45"]
["","","","Mittel","dB(A)","","","","","38","","41"]
["","","","Niedrig","dB(A)","","","","","33","","36"]
["","","","Flüsterbetrieb","dB(A)","","","","","30","","33"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","","","","","6.35","","6.35"]
["","Gas","","AD","mm","","","","","12.7","","12.7"]
["","Drain","","","","","","","","18","","18"]
["Regelungssysteme","Infrared remote control","","","","","","","","ARC470A1","","ARC470A1"]
["","Wired remote control","","","","","","","","BRC073A1","","BRC073A1"]
["Standardzubehör","Trockenbatterien, Typ AAA","","","","","","","","2","","2"]
["","Installationsanleitung","","","","","","","","1","","1"]
["","Bedienungsanleitung","","","","","","","","1","","1"]
["","Infrarot-Fernbedienung","","","","","","","","1","","1"]
["","Fernbedienungshalterung","","","","","","","","1","","1"]
["","Montageplatte","","","","","","","","1","","1"]
["","Befestigungsschrauben für Hauptgerät","","","","","","","","2","","2"]
["Power supply","Bezeichnung","","","","","","","","V1","","V1"]
["","Phase","","","","","","","","1~","","1~"]
["","Frequenz","","","Hz","","","","","50","","50"]
["","Spannung","","","V","","","","","220-240","","220-240"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","0.023","0.023","0.029","0.040","","0.032"]
["","Heizen","","Nom.","kW","0.023","0.023","0.029","0.040","","0.035"]
["Gehäuse","Farbe","","","","Weiß","Weiß","Weiß","Weiß","","Weiß"]
["Abmessungen","Maßeinheit","","Höhe","mm","286","286","286","286","","295"]
["","","","Breite","mm","770","770","770","770","","990"]
["","","","Tiefe","mm","225","225","225","225","","263"]
["Gewicht","Maßeinheit","","","kg","8","8","8.5","9.00","","13.5"]
["Ventilator","Luftstromvolumen","Kühlung","Hoch","m³/min","9.8","10","11.5","12.6","","17.3"]
["","","Kühlen","Mittel","m³/min","8","8","8","9","","14.8"]
["","","","Niedrig","m³/min","6","6.2","6.4","6.9","","12.2"]
["","","","Flüsterbetrieb","m³/min","4.3","4.3","4.4","4.9","","10.7"]
["","","Heizen","Hoch","m³/min","10.4","10.4","11.9","12.8","","17.9"]
["","","","Mittel","m³/min","8.3","8.4","8.6","8.8","","15.8"]
["","","","Niedrig","m³/min","6.2","6.4","6.5","6.7","","12.8"]
["","","","Flüsterbetrieb","m³/min","5.3","5.3","5.3","5.2","","11.3"]
["Schallleistungspegel","Kühlung","","","dB(A)","53","54","54","59.0","","60"]
["","Heizen","","","dB(A)","55","55","56","59.0","","62"]
["Schalldruckpegel","Kühlung","","Hoch","dB(A)","39","40","43","45.0","","45"]
["","Kühlen","","Mittel","dB(A)","33","33","34","36.0","","41"]
["","","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dB(A)","25","26","27","30.0","","36"]
["","","","Flüsterbetrieb","dB(A)","20","20","20","22.0","","33"]
["","Heizen","","Hoch","dB(A)","39","40","40","44.0","","44"]
["","","","Mittel","dB(A)","34","34","35","34.0","","40"]
["","","","Niedrig","dB(A)","28","28","29","28.0","","35"]
["","","","Flüsterbetrieb","dB(A)","21","21","21","22.0","","32"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","6","6","6","6","","6.35"]
["","Gas","","AD","mm","9.5","9.5","9.5","9.50","","12.7"]
["","Ableitung","","","","18","18","18","18","","18"]
["Regelungssysteme","Infrarot-Fernbedienung","","","","ARC470A1","ARC470A1","ARC470A1","ARC470A1","","ARC470A1"]
["","Verkabelte Fernbedienung","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","","BRC073A1"]
["Standardzubehör","Installation manual","","","","1","1","1","1","","1"]
["","AAA dry-cell batteries","","","","2","2","2","2","","2"]
["","General safety precautions","","","","196","196","196","196"]
["","Operation manual","","","","1","1","1","1","","1"]
["","Batteries","","","","1","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2","2","","2"]
["","Infrared remote control","","","","1","1","1","1","","1"]
["","Mounting plate","","","","1","1","1","1","","1"]
["","Remote control holder","","","","1","1","1","1","","1"]
["Stromversorgung","Phase","","","","1~","1~","1~","1~","","1~"]
["","Frequenz","","","Hz","50","50","50","50","","50"]
["Spannungsversorgung","Spannung","","","V","220-440","220-440","220-440","220-440","","220-240"]
["Stromversorgung","Bezeichnung","","","","","","","","","V1"]