{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":7,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXG-JB / RXG-K"]
[]
[]
[]
[]
["","","","","FTXG25JV1BB / RXG25K3V1B","FTXG35JV1BB / RXG35K3V1B","FTXG50JV1BB / RXG50K3V1B"]
["Kühlleistung","Min.","","kW","1.3","1.4","1.7"]
["","Max.","","kW","3.0","3.8","5.3"]
["","Nom.","","kW","2.5 (2)","3.5 (2)","5.0 (2)"]
["Rohrleitungsanschlüsse","Liquid","OD","mm","6.35","6.35","6.35"]
["","Gas","AD","mm","9.52","9.52","12.7"]
["","Drain","AD","mm","16 oder 18","16 oder 18","18.0"]
["Nominale Effizienz","Jährlicher Energieverbrauch","","kWh","280","445","780"]
["","EER","","","4.46 (1)","3.93 (1)","3.21 (1)"]
["","COP","","","4.36 (1)","4.04 (1)","3.63 (1)"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","A","A","A"]
["","","Heizen","","A","A","A"]
["Heizleistung","Nom.","","kW","3.4 (3)","4.0 (3)","5.8 (3)"]
["","Min.","","kW","1.3","1.4","1.7"]
["","Max.","","kW","4.5","5.0","6.5"]
["Hinweise","","","","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU"]
["","","","","(2) - Kühlen: Innentemperatur: 27°C TK, 19,0°C FK; Außentemp. 35°C TK, 24°C FK; äquivalente Leitungslänge: 5 m","(2) - Kühlen: Innentemperatur: 27°C TK, 19,0°C FK; Außentemp. 35°C TK, 24°C FK; äquivalente Leitungslänge: 5 m","(2) - Kühlen: Innentemperatur: 27°C TK, 19,0°C FK; Außentemp. 35°C TK, 24°C FK; äquivalente Leitungslänge: 5 m"]
["","","","","(3) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m","(3) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m","(3) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m"]
["","","","","(4) - 220 V","(4) - 220 V","(4) - 220 V"]
["","","","","(5) - 230 V","(5) - 230 V","(5) - 230 V"]
["","","","","(6) - 240 V","(6) - 240 V","(6) - 240 V"]
["","","","","(7) - Nominale Effizienz: Kühlen bei 35 °C/27 °C Nennlast, Heizen bei 7 °C/20 °C Nennlast","(7) - Nominale Effizienz: Kühlen bei 35 °C/27 °C Nennlast, Heizen bei 7 °C/20 °C Nennlast","(7) - Nominale Effizienz: Kühlen bei 35 °C/27 °C Nennlast, Heizen bei 7 °C/20 °C Nennlast"]