{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":7,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXG-JB"]
[]
[]
[]
[]
["","","","","FTXG25JV1BB","FTXG35JV1BB","FTXG50JV1BB"]
["Schalldruckpegel","Heizen","Hoch","dBA","39","42","44"]
["","","Flüsterbetrieb","dBA","25","26","32"]
["","","Niedrig","dBA","28","29","35"]
["","Kühlung","Flüsterbetrieb","dBA","22","23","32"]
["","","Niedrig","dBA","25","26","35"]
["","","Hoch","dBA","38","42","44"]
["","","Nom.","dBA","34","36","40"]
["","Kühlung","Nom.","dBA","32","34","40"]
["Standardzubehör","Fotokatalytischer Luftreinigungsfilter mit Titanapatit","","","2","2","2"]
["","Bedienungsanleitung","","","1","1","1"]
["","Installationsanleitung","","","1","1","1"]
["","Infrarotfernbedienung","","","1","1","1"]
["","Batterien","","","2","2","2"]
["","Fernbedienungshalterung","","","1","1","1"]
["","Befestigungsschrauben für Hauptgerät","","","2","2","2"]
["","Montageplatte","","","1","1","1"]
["","Papierschablone","","","2","2","2"]
["Rohrleitungsanschlüsse","Flüssigkeit","AD","mm","6.35","6.35","6.35"]
["","Gas","AD","mm","9.52","9.52","12.7"]
["","Ableitung","","","16 oder 18","16 oder 18","18"]
["Leistungsaufnahme","Kühlung","Nom.","kW","0.018 (3), 0.018 (4), 0.018 (5)","0.026 (3), 0.026 (4), 0.026 (5)","0.032 (3), 0.032 (4), 0.032 (5)"]
["","Heizen","Nom.","kW","0.024 (3), 0.024 (4), 0.024 (5)","0.032 (3), 0.032 (4), 0.032 (5)","0.038 (3), 0.038 (4), 0.038 (5)"]
["Schallleistungspegel","Kühlung","","dBA","56","60","60"]
["","Heizen","","dBA","57","60","60"]
["Abmessungen","Maßeinheit","Breite","mm","915","915","915"]
["","","Tiefe","mm","155","155","155"]
["","","Höhe","mm","295","295","295"]
["Gehäuse","Farbe","","","Schwarzmatt","Schwarzmatt","Schwarzmatt"]
["Gewicht","Maßeinheit","","kg","11","11","11"]
["Power supply","Phase","","","1~","1~","1~"]
["","Frequenz","","Hz","50","50","50"]
["","Bezeichnung","","","V1","V1","V1"]
["","Spannung","","V","220-240","220-240","220-240"]
["Hinweise","","","","(1) - SL: Die flüsterleise Ventilatorstufe der Luftmengeneinstellung.","(1) - SL: Die flüsterleise Ventilatorstufe der Luftmengeneinstellung.","(1) - SL: Die flüsterleise Ventilatorstufe der Luftmengeneinstellung."]
["","","","","(2) - Bei Anschluss an einem Multi-Außengerät lesen Sie bitte die technischen Gerätedaten des anzuschließenden Multi-Außengeräts.","(2) - Bei Anschluss an einem Multi-Außengerät lesen Sie bitte die technischen Gerätedaten des anzuschließenden Multi-Außengeräts.","(2) - Bei Anschluss an einem Multi-Außengerät lesen Sie bitte die technischen Gerätedaten des anzuschließenden Multi-Außengeräts."]
["","","","","(3) - 220 V","(3) - 220 V","(3) - 220 V"]
["","","","","(4) - 230 V","(4) - 230 V","(4) - 230 V"]
["","","","","(5) - 240 V","(5) - 240 V","(5) - 240 V"]