{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":6,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXG-LW / RXLG-M"]
[]
[]
[]
[]
["","","","","FTXG25LV1BW / RXLG25M2V1B","FTXG35LV1BW / RXLG35M2V1B"]
["Outdoor unit","","","","RXLG25M","RXLG35M"]
["Kühlleistung","Min.","","kW","1.3","1.4"]
["","Nom.","","kW","2.5","3.5"]
["","Max.","","kW","4.0","4.6"]
["Heizleistung","Min.","","kW","1.0","1.0"]
["","Nom.","","kW","4.4","5.1"]
["","Max.","","kW","6.1, 3.6","6.7, 4.2"]
["Nominale Effizienz","EER","","","3.68","3.57"]
["","COP","","","4.31","3.89"]
["","Jährlicher Energieverbrauch","","kWh","340","490"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","A","A"]
["","","Heizen","","A","A"]
["Rohrleitungsanschlüsse","Ableitung","AD","mm","18","18"]
["","Gas","AD","mm","9.5","9.5"]
["","Flüssigkeit","AD","mm","6.35","6.35"]
["Raumkühlen","Energieeffizienzklasse","","","A++","A++"]
["","Leistung","Pdesign","kW","2.50","3.50"]
["","SEER","","","7.04","6.67"]
["","Jährlicher Energieverbrauch","","kWh/a","124","184"]
["Raumheizen (Durchschnittliches Klima)","Energieeffizienzklasse","","","A++","A++"]
["","Leistung","Pdesign","kW","2.50","3.00"]
["","SCOP/A","","","4.64","4.60"]
["","Jährlicher Energieverbrauch","","kWh/a","755","913"]
["Hinweise","","","","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU"]
["","","","","(2) - Nominale Effizienz: Kühlen bei 35°C/27°C Nennlast, Heizen bei 7°C/20°C Nennlast","(2) - Nominale Effizienz: Kühlen bei 35°C/27°C Nennlast, Heizen bei 7°C/20°C Nennlast"]
["","","","","(3) - 220V","(3) - 220V"]
["","","","","(4) - 230V","(4) - 230V"]
["","","","","(5) - 240V","(5) - 240V"]
["","","","","(6) - Für minimale Nenn-Heizleistung ist Innengerätventilator auf SL eingestellt","(6) - Für minimale Nenn-Heizleistung ist Innengerätventilator auf SL eingestellt"]
["","","","","(7) - Maximale Heizleistung bei -15°C Außentemperatur","(7) - Maximale Heizleistung bei -15°C Außentemperatur"]