{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":8,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-AS"]
[]
[]
[]
[]
["","","","","","FTXJ20A2V1BS","FTXJ35A2V1BS","FTXJ42A2V1BS"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","0.02","0.024","0.028"]
["","Heizen","","Nom.","kW","0.021","0.024","0.036"]
["Gehäuse","Farbe","","","","Silbern","Silbern","Silbern"]
["Abmessungen","Maßeinheit","","Höhe","mm","305","305","305"]
["","","","Breite","mm","900","900","900"]
["","","","Tiefe","mm","212","212","212"]
["Gewicht","Maßeinheit","","","kg","12","12","12"]
["Ventilator","Luftstromvolumen","Kühlung","Hoch","m³/min","11","11.8","13"]
["","","Kühlen","Mittel","m³/min","8.4","8.6","9.5"]
["","","","Niedrig","m³/min","6","6","7.2"]
["","","","Flüsterbetrieb","m³/min","4.6","4.6","4.6"]
["","","Heizen","Hoch","m³/min","11.1","11.7","14.4"]
["","","","Mittel","m³/min","8.7","9","10.5"]
["","","","Niedrig","m³/min","6.4","6.4","7.7"]
["","","","Flüsterbetrieb","m³/min","4.6","4.6","5.2"]
["Schallleistungspegel","Kühlung","","","dB(A)","57","60","60"]
["Schalldruckpegel","Kühlung","","Hoch","dB(A)","39","41","45"]
["","Kühlen","","Mittel","dB(A)","32","33","37"]
["","","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dB(A)","25","25","29"]
["","","","Flüsterbetrieb","dB(A)","19","19","21"]
["","Heizen","","Hoch","dB(A)","39","41","45"]
["","","","Mittel","dB(A)","32","33","37"]
["","","","Niedrig","dB(A)","25","25","29"]
["","","","Flüsterbetrieb","dB(A)","19","19","21"]
["Kältemittel","GWP","","","","675","675","675"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","6.35","6.35","6.35"]
["","Gas","","AD","mm","9.5","9.5","12.7"]
["","Ableitung","","","","18","18","18"]
["Regelungssysteme","Infrared remote control","","","","ARC488A1S","ARC488A1S","ARC488A1S"]
["Regelungssysteme","Verkabelte Fernbedienung","","","","BRC073A1","BRC073A1","BRC073A1"]
["Standardzubehör","Installation manual","","","","1","1","1"]
["","Wireless remote control","","","","1","1","1"]
["","Screw cover","","","","2","2","2"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","General safety precautions","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1","1"]
["","Silver particle filter","","","","1","1","1"]
["","Mounting plate","","","","1","1","1"]
["","Remote control holder","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Stromversorgung","Bezeichnung","","","","V1","V1","V1"]
["","Phase","","","","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50"]
["Spannungsversorgung","Spannung","","","V","220-240","220-240","220-240"]