{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":8,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-AW / RXJ-M9"]
[]
[]
[]
[]
["","","","","FTXJ35A2V1BW  / RXJ35M5V1B9","FTXJ20A2V1BW / RXJ20M5V1B9","FTXJ25A2V1BW / RXJ25M5V1B9","FTXJ35A2V1BW / RXJ35M5V1B9"]
["Kühlleistung","Nom.","","kW","3.50"]
["Nominale Effizienz","Jährlicher Energieverbrauch","","kWh","428"]
["","EER","","","4.09"]
["","COP","","","4.04"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","A"]
["","","Heizen","","A"]
["Heizleistung","Nom.","","kW","4.00"]
["Hinweise","","","","(1) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","(2) - Siehe separate Zeichnung für die elektrischen Daten"]
["","","","","(3) - Nennkühlleistungen basieren auf: Innentemperatur: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m."]
["","","","","(4) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m."]
["Außengerät","","","","","RXJ20M5V1B9","RXJ25M5V1B9","RXJ35M5V1B9"]
["Kühlleistung","Nom.","","kW","","2.30","2.40","3.50"]
["Heizleistung","Nom.","","kW","","2.50","3.20","4.00"]
["Nominale Effizienz","EER","","","","4.64","4.73","4.09"]
["","COP","","","","5.00","4.57","4.04"]
["","Jährlicher Energieverbrauch","","kWh","","248","254","428"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","","A","A","A"]
["","","Heizen","","","A","A","A"]
["Raumkühlen","Energieeffizienzklasse","","","","A+++","A+++","A++"]
["","Leistung","Pdesign","kW","","2.30","2.40","3.50"]
["","SEER","","","","8.73","8.64","7.19"]
["","Jährlicher Energieverbrauch","","kWh/a","","92","97","170"]
["Raumheizen (Durchschnittliches Klima)","Energieeffizienzklasse","","","","A++","A++","A++"]
["","Leistung","Pdesign","kW","","2.10","2.70","3.00"]
["","SCOP/A","","","","4.61","4.60","4.60"]
["","Raumheizen (Durchschnittliches Klima)-=-Heizleistung Pdh bei -10°-=-kW","","kW","","1.80","2.18","2.61"]
["","Jährlicher Energieverbrauch","","kWh/a","","638","822","913"]
["Energy Efficiency Range","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]