{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":5,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MS / 4MXM-A8"]
[]
[]
[]
[]
["","","","","FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / 4MXM80A2V1B8"]
["Kühlleistung","Nom.","","kW","7.50"]
["Heizleistung","Nom.","","kW","10.00"]
["Nominale Effizienz","EER","","","4.13"]
["","COP","","","3.32"]
["","Jährlicher Energieverbrauch","","kWh","908"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","A"]
["","","Heizen","","C"]
["Raumkühlen","Energieeffizienzklasse","","","A++"]
["","Leistung","Pdesign","kW","7.50"]
["","SEER","","","6.92"]
["","Jährlicher Energieverbrauch","","kWh/a","380"]
["Raumheizen (Durchschnittliches Klima)","Energieeffizienzklasse","","","A+"]
["","Leistung","Pdesign","kW","6.46"]
["","SCOP/A","","","4.02"]
["","Raumheizen (Durchschnittliches Klima)-=-Heizleistung Pdh bei -10°-=-kW","","kW","5.28"]
["","Jährlicher Energieverbrauch","","kWh/a","2,245"]
["Hinweise","","","","(1) - Nennkühlleistungen basieren auf: Innentemp.: 27°CTK, 19°CFK; Außentemperatur: 35°CTK; äquivalente Länge Kältemittelleitung: 5m; Niveauunterschied: 0m."]
["","","","","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5m; Niveauunterschied: 0 m."]
["","","","","(3) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","(4) - Siehe separate Zeichnung für die elektrischen Daten"]