{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":9,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MW / 3MXM-N"]
[]
[]
[]
[]
["","","","","FTXJ20MV1BW / FTXJ20MV1BW / FTXJ20MV1BW / 3MXM40N2V1B","FTXJ20MV1BW / FTXJ20MV1BW / 3MXM40N2V1B","FTXJ20MV1BW / FTXJ20MV1BW / 3MXM52N2V1B","FTXJ20MV1BW / FTXJ20MV1BW / FTXJ20MV1BW / 3MXM52N2V1B","FTXJ20MV1BW / FTXJ20MV1BW / FTXJ20MV1BW / 3MXM68N2V1B"]
["Kühlleistung","Nom.","","kW","4.00","","4.00","5.20","6.00"]
["Nominale Effizienz","Jährlicher Energieverbrauch","","kWh","467","","471","593","787"]
["","EER","","","4.28","","4.25","4.38","3.81"]
["","COP","","","4.32","","4.05","4.42","3.88"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","A","","A","A","A"]
["","","Heizen","","A","","A","A","A"]
["Heizleistung","Nom.","","kW","4.60","","6.80","6.80","7.80"]
["Kühlleistung","Nom.","","kW","","4.00"]
["Heizleistung","Nom.","","kW","","4.60"]
["Nominale Effizienz","EER","","","","4.15"]
["","COP","","","","3.95"]
["","Jährlicher Energieverbrauch","","kWh","","482"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","","A"]
["","","Heizen","","","A"]
["Raumkühlen","Energieeffizienzklasse","","","","A++"]
["","Leistung","Pdesign","kW","","4.00"]
["","SEER","","","","7.62"]
["","Jährlicher Energieverbrauch","","kWh/a","","164"]
["Raumheizen (Durchschnittliches Klima)","Energieeffizienzklasse","","","","A+"]
["","Leistung","Pdesign","kW","","4.80"]
["","SCOP/A","","","","4.11"]
["","Raumheizen (Durchschnittliches Klima)-=-Heizleistung Pdh bei -10°-=-kW","","kW","","3.58"]
["","Jährlicher Energieverbrauch","","kWh/a","","1632"]
["Hinweise","","","","","(1) - Nennkühlleistungen basieren auf: Innentemp.: 27°CTK, 19°CFK; Außentemperatur: 35°CTK; äquivalente Länge Kältemittelleitung: 5m; Niveauunterschied: 0m."]
["","","","","","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5m; Niveauunterschied: 0 m."]
["","","","","","(3) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","","(4) - Siehe separate Zeichnung für die elektrischen Daten"]