{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":14,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-M / 4MXM-N"]
[]
[]
[]
[]
["","","","","FTXM20M2V1B / FTXM50M2V1B / 4MXM68N2V1B","FTXM35M2V1B / FTXM35M2V1B / 4MXM68N2V1B","FTXM20M2V1B / FTXM20M2V1B / FTXM25M2V1B / 4MXM68N2V1B","FTXM20M2V1B / FTXM25M2V1B / FTXM25M2V1B / 4MXM68N2V1B","FTXM25M2V1B / FTXM42M2V1B / 4MXM68N2V1B","FTXM20M2V1B / FTXM20M2V1B / FTXM42M2V1B / 4MXM80N2V1B","FTXM20M2V1B / FTXM25M2V1B / FTXM35M2V1B / 4MXM80N2V1B","FTXM20M2V1B / FTXM20M2V1B / FTXM20M2V1B / FTXM20M2V1B / 4MXM80N2V1B","FTXM20M2V1B / FTXM60M2V1B / 4MXM80N2V1B","FTXM35M2V1B / FTXM42M2V1B / 4MXM80N2V1B"]
["Kühlleistung","Nom.","","kW","6.8","6.8","6.5","6.8","6.7","8.00","7.40","7.40","7.40","7.70"]
["Raumkühlen","SEER","","","7.78","8.02","7.76","7.71","7.99","8.07","8.19","8.32","7.38","7.40"]
["","Jährlicher Energieverbrauch","","kWh/a","306","297","294","309","294","356","317","311","351","365"]
["","Leistung","Pdesign","kW","6.80","6.80","6.50","6.80","6.70","8.20","7.40","7.40","7.40","7.70"]
["","Energieeffizienzklasse","","","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++"]
["Raumheizen (Durchschnittliches Klima)","Leistung","Pdesign","kW","4.50","4.80","5.30","5.30","4.30","5.37","5.37","6.23","4.27","4.27"]
["","SCOP/A","","","3.90","4.00","4.09","4.10","3.86","3.93","3.95","4.55","4.05","4.05"]
["","Energieeffizienzklasse","","","A","A+","A+","A+","A","A","A","A+","A+","A+"]
["","Jährlicher Energieverbrauch","","kWh/a","1,612","1,680","1,814","1,807","1,559","1,913","1,902","1,915","1,474","1,475"]
["Nominale Effizienz","Jährlicher Energieverbrauch","","kWh","794","723","810","883","751","874","749","810","803","841"]
["","EER","","","4.28","4.70","4.01","3.85","4.46","4.58","4.94","4.57","4.61","4.58"]
["","COP","","","3.82","3.81","4.49","4.38","3.95","3.91","3.90","4.97","3.85","3.35"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","A","A","A","A","A","A","A","A","A","A"]
["","","Heizen","","A","A","A","A","A","A","A","A","A","C"]
["Heizleistung","Nom.","","kW","8.60","8.60","8.20","8.60","8.30","9.40","9.30","9.60","9.30","9.00"]
["Hinweise","","","","(1) - Siehe separate Zeichnung für die elektrischen Daten","(1) - Siehe separate Zeichnung für die elektrischen Daten","(1) - Siehe separate Zeichnung für die elektrischen Daten","(1) - Siehe separate Zeichnung für die elektrischen Daten","(1) - Siehe separate Zeichnung für die elektrischen Daten","(1) - Siehe separate Zeichnung für die elektrischen Daten","(1) - Siehe separate Zeichnung für die elektrischen Daten","(1) - Siehe separate Zeichnung für die elektrischen Daten","(1) - Siehe separate Zeichnung für die elektrischen Daten","(1) - Siehe separate Zeichnung für die elektrischen Daten"]