{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":10,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-M / RXM-M9"]
[]
[]
[]
[]
["","","","","FTXM20M2V1B / RXM20M3V1B9","FTXM25M2V1B / RXM25M3V1B9","FTXM35M2V1B / RXM35M3V1B9","FTXM42M2V1B / RXM42M3V1B9","FTXM50M2V1B / RXM50M3V1B9","FTXM60M2V1B / RXM60M3V1B9"]
["Kühlleistung","Min.","","kW","1.3"]
["","Max.","","kW","2.6"]
["","Nom.","","kW","2.0"]
["Nominale Effizienz","Jährlicher Energieverbrauch","","kWh","220"]
["","EER","","","4.57"]
["","COP","","","5.00"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","A"]
["","","Heizen","","A"]
["Heizleistung","Nom.","","kW","2.50"]
["","Min.","","kW","1.30"]
["","Max.","","kW","3.50"]
["Hinweise","","","","(1) - Siehe separate Zeichnung für die elektrischen Daten"]
["","","","","(2) - Nennkühlleistungen basieren auf: Innentemp.: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m."]
["","","","","(3) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m."]
["Außengerät","","","","","RXM25M3V1B9","RXM35M3V1B9","RXM42M3V1B9","RXM50M3V1B9","RXM60M3V1B9"]
["Kühlleistung","Min.","","kW","","1.3","1.4","1.70","1.70","1.90"]
["","Nom.","","kW","","2.5","3.4","4.20","5.00","6.00"]
["","Max.","","kW","","3.2","4.0","5.00","5.30","6.70"]
["Heizleistung","Min.","","kW","","1.30","1.40","1.70","1.70","1.70"]
["","Nom.","","kW","","2.80","4.00","5.40","5.80","7.00"]
["","Max.","","kW","","4.70","5.20","6.00","6.50","8.00"]
["Nominale Effizienz","EER","","","","4.50","4.23","3.75","3.68","3.39"]
["","COP","","","","5.00","4.04","4.12","4.00","3.61"]
["","Jährlicher Energieverbrauch","","kWh","","280","400"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","","A","A","A","A","A"]
["","","Heizen","","","A","A","A","A","A"]
["Raumkühlen","Energieeffizienzklasse","","","","A+++","A+++","A++","A++","A++"]
["","Leistung","Pdesign","kW","","2.50","3.40","4.20","5.00","6.00"]
["","SEER","","","","8.52","8.51","7.50","7.33","6.90"]
["","Jährlicher Energieverbrauch","","kWh/a","","103","140","196","239","304"]
["Raumheizen (Durchschnittliches Klima)","Energieeffizienzklasse","","","","A+++","A+++","A++","A++","A+"]
["","Leistung","Pdesign","kW","","2.40","2.50","4.00","4.60","4.60"]
["","SCOP/A","","","","5.10","5.10","4.60","4.60","4.30"]
["","Raumheizen (Durchschnittliches Klima)-=-Heizleistung Pdh bei -10°-=-kW","","kW","","2.30","2.35","3.68","4.09","4.09"]
["","Jährlicher Energieverbrauch","","kWh/a","","659","686","1216","1400","1496"]