{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":8,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-M / RXM-N"]
[]
[]
[]
[]
["","","","","FTXM42M2V1B / RXM42N2V1B","FTXM50M2V1B / RXM50N2V1B","FTXM60M2V1B / RXM60N2V1B","FTXM71M2V1B / RXM71N2V1B"]
["Kühlleistung","Min.","","kW","1.70","1.70"]
["","Max.","","kW","5.00","5.30"]
["","Nom.","","kW","4.20","5.00"]
["Nominale Effizienz","EER","","","3.75","3.68"]
["","COP","","","4.12","4.00"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","A","A"]
["","","Heizen","","A","A"]
["Heizleistung","Nom.","","kW","5.40","5.80"]
["","Min.","","kW","1.70","1.70"]
["","Max.","","kW","6.00","6.50"]
["Hinweise","","","","(1) - Siehe separate Zeichnung für die elektrischen Daten","(1) - Siehe separate Zeichnung für die elektrischen Daten"]
["","","","","(2) - Nennkühlleistungen basieren auf: Innentemp.: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m.","(2) - Nennkühlleistungen basieren auf: Innentemp.: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m."]
["","","","","(3) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m.","(3) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m."]
["Outdoor unit","","","","","","RXM60N2V1B","RXM71N2V1B"]
["Kühlleistung","Min.","","kW","","","1.90","2.30"]
["","Nom.","","kW","","","6.00","7.10"]
["","Max.","","kW","","","6.70","8.50"]
["Heizleistung","Min.","","kW","","","1.70","2.30"]
["","Nom.","","kW","","","7.00","8.20"]
["","Max.","","kW","","","8.00","10.20"]
["Nominale Effizienz","EER","","","","","3.39","3.03"]
["","COP","","","","","3.61","3.19"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","","","A","B"]
["","","Heizen","","","","A","D"]
["Raumkühlen","Energieeffizienzklasse","","","","","A++","A++"]
["","Leistung","Pdesign","kW","","","6.00","7.10"]
["","SEER","","","","","6.90","6.11"]
["","Jährlicher Energieverbrauch","","kWh/a","","","304","407"]
["Raumheizen (Durchschnittliches Klima)","Energieeffizienzklasse","","","","","A+","A"]
["","Leistung","Pdesign","kW","","","4.60","6.20"]
["","SCOP/A","","","","","4.30","3.81"]
["","Raumheizen (Durchschnittliches Klima)-=-Heizleistung Pdh bei -10°-=-kW","","kW","","","4.09","5.01"]
["","Jährlicher Energieverbrauch","","kWh/a","","","1496","2276"]
["Nominale Effizienz","Jährlicher Energieverbrauch","","kWh","","","","1170"]