{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":8,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXN-MB9"]
[]
[]
[]
[]
["","","","","FTXN25MV1B9","FTXN35MV1B9","FTXN50MV1B9","FTXN60MV1B9"]
["Schalldruckpegel","Heizen","Hoch","dB(A)","40","41","40","43"]
["","","Flüsterbetrieb","dB(A)","21","22","32","33"]
["","","Niedrig","dB(A)","29","30","35","37"]
["","Kühlung","Flüsterbetrieb","dB(A)","21","22","32","33"]
["","","Besonders hoch","dB(A)","41","42","44","46"]
["","","Niedrig","dB(A)","29","30","35","37"]
["","","Hoch","dB(A)","40","41","40","43"]
["","","Nom.","dB(A)","34","34","38","41"]
["","Kühlung","Nom.","dB(A)","34","34","38","41"]
["Regelungssysteme","Infrared remote control","","","APGS02","APGS02","APGS02","APGS02"]
["Rohrleitungsanschlüsse","Flüssigkeit","AD","mm","6.35","6.35","6.35","6.35"]
["","Gas","AD","mm","9.52","9.52","12.70","15.90"]
["","Ableitung","","","19.05","19.05","19.05","19.05"]
["Sound power level","Kühlung","","dB(A)","53","54","55","61"]
["Abmessungen","Maßeinheit","Breite","mm","800","800","1,065","1,065"]
["","","Tiefe","mm","206","206","224","224"]
["","","Höhe","mm","288","288","310","310"]
["Gehäuse","Farbe","","","Weiß","Weiß","Weiß","Weiß"]
["Gewicht","Maßeinheit","","kg","9","9","14","14"]
["Power supply","Phase","","","1~","1~","1~","1~"]
["","Frequenz","","Hz","50","50","50","50"]
["","Bezeichnung","","","V1","V1","V1","V1"]
["","Spannung","","V","220-240","220-240","220-240","220-240"]
["Hinweise","","","","(1) - Alle Geräte sind getestet und entsprechen ISO 5151 (Gerät ohne Kanal) oder ISO 13253 (Gerät mit Kanal).","(1) - Alle Geräte sind getestet und entsprechen ISO 5151 (Gerät ohne Kanal) oder ISO 13253 (Gerät mit Kanal).","(1) - Alle Geräte sind getestet und entsprechen ISO 5151 (Gerät ohne Kanal) oder ISO 13253 (Gerät mit Kanal).","(1) - Alle Geräte sind getestet und entsprechen ISO 5151 (Gerät ohne Kanal) oder ISO 13253 (Gerät mit Kanal)."]
["","","","","(2) - Änderungen aller Technischen Daten durch den Hersteller ohne Ankündigung vorbehalten.","(2) - Änderungen aller Technischen Daten durch den Hersteller ohne Ankündigung vorbehalten.","(2) - Änderungen aller Technischen Daten durch den Hersteller ohne Ankündigung vorbehalten.","(2) - Änderungen aller Technischen Daten durch den Hersteller ohne Ankündigung vorbehalten."]