{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":57,"n_cols":11,"rows_kept":57,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-N"]
[]
[]
[]
[]
["","","","","","FTXP35N5V1B","FTXP50N2V1B","FTXP60N2V1B","FTXP71N2V1B","FTXP20N5V1B (Archived)","FTXP25N5V1B (Archived)"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","0.032","0.029","0.032","0.032","0.019","0.02"]
["","Heizen","","Nom.","kW","0.032","0.032","0.035","0.035","0.023","0.023"]
["Gehäuse","Farbe","","","","Weiß","Weiß","Weiß","Weiß","Weiß","Weiß"]
["Abmessungen","Maßeinheit","","Höhe","mm","286","295","295","295","286","286"]
["","","","Breite","mm","770","990","990","990","770","770"]
["","","","Tiefe","mm","225","263","263","263","225","225"]
["Gewicht","Maßeinheit","","","kg","9","13.5","13.5","13.5","8.5","8.5"]
["Ventilator","Luftstromvolumen","Kühlung","Hoch","m³/min","11.5","16.3","16.8","16.8","9.5","9.7"]
["","","Kühlen","Mittel","m³/min","8.3","14","14.4","14.4","7.4","7.7"]
["","","","Niedrig","m³/min","6.3","11.5","11.8","11.8","5.6","5.8"]
["","","","Flüsterbetrieb","m³/min","4.5","8.3","9.2","10.1","4.2","4.2"]
["","","Heizen","Hoch","m³/min","11.5","17.3","17.9","17.9","10.4","10.4"]
["","","","Mittel","m³/min","9","14.4","15.3","15.3","8.1","8.1"]
["","","","Niedrig","m³/min","7","11.8","12.4","12.4","6.2","6.4"]
["","","","Flüsterbetrieb","m³/min","5.3","10.4","11","11","5.2","5.2"]
["Schallleistungspegel","Kühlung","","","dB(A)","58","59","60","62","55","55"]
["","Heizen","","","dB(A)","58","61","62","62","55","55"]
["Schalldruckpegel","Kühlung","","Hoch","dB(A)","43","43","45","46","39","40"]
["","Kühlen","","Mittel","dB(A)","34","39","41","42"]
["","","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dB(A)","27","34","36","37","25","26"]
["","","","Flüsterbetrieb","dB(A)","20","27","30","32","19","19"]
["","Heizen","","Hoch","dB(A)","40","42","44","45","39","40"]
["","","","Mittel","dB(A)","35","38","40","41"]
["","","","Niedrig","dB(A)","29","33","35","36","28","28"]
["","","","Flüsterbetrieb","dB(A)","21","30","32","33","21","21"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","6","6.4","6.4","6.4","6","6"]
["","Gas","","AD","mm","9.5","12.7","12.7","12.7","9.5","9.5"]
["","Ableitung","","","","18","18","18","18","18","18"]
["Regelungssysteme","Infrared remote control","","","","ARC480A78","ARC480A53","ARC480A53","ARC480A53"]
["Regelungssysteme","Verkabelte Fernbedienung","","","","BRC944B2, BRC073A1","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Standardzubehör","Installation manual","","","","1","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2","2","2"]
["","General safety precautions","","","","1","","","","1","1"]
["","Operation manual","","","","1","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1","1","1","1","1"]
["","Silver particle filter","","","","1","1","1","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1","1"]
["Stromversorgung","Bezeichnung","","","","","V1","V1","V1"]
["","Phase","","","","1~","1~","1~","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50","50","50","50"]
["Spannungsversorgung","Spannung","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Standardzubehör","WLAN adapter kit","","","","","1","1","1"]
["Schalldruckpegel","Kühlen","","Schalldruckpegel-=-Kühlen-=-Mittel-=-dB(A)","dB(A)","","","","","33","33"]
["","Heizen","","Schalldruckpegel-=-Heizen-=-Mittel-=-dB(A)","dB(A)","","","","","34","34"]
["Regelungssysteme","Infrarot-Fernbedienung","","","","","","","","ARC480A78","ARC480A78"]
["Hinweise","","","","","","","","","(1) - Kühlen: Innentemperatur: 27°C TK, 19°C FK, Außentemp. 35°C TK, äquivalente Leitungslänge: 5 m; Niveauunterschied: 0 m","(1) - Kühlen: Innentemperatur: 27°C TK, 19°C FK, Außentemp. 35°C TK, äquivalente Leitungslänge: 5 m; Niveauunterschied: 0 m"]
["","","","","","","","","","(2) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m (horizontal)","(2) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m (horizontal)"]
["","","","","","","","","","(3) - Siehe separate Zeichnung für die elektrischen Daten","(3) - Siehe separate Zeichnung für die elektrischen Daten"]