{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":12,"n_cols":8,"rows_kept":12,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-K1 / RXS-L1"]
[]
[]
[]
[]
["","","","FTXS20K3V1B1 / RXS20L3V1B1","FTXS25K3V1B1 / RXS25L3V1B1","FTXS35K3V1B1 / RXS35L3V1B1","FTXS42K3V1B1 / RXS42L2V1B1","FTXS50K3V1B1 / RXS50L2V1B1"]
["Kühlleistung","Nom.","kW","2.00 (1)","2.50 (1)","3.25 (1)","4.20 (1)","4.50 (1)"]
["Nominale Effizienz","EER","","4.29","4.12","3.87","3.75","3.65"]
["","COP","","4.60","4.45","4.40","3.93","3.83"]
["Heizleistung","Nom.","kW","2.50 (2)","2.85 (2)","3.80 (2)","5.35 (2)","5.65 (2)"]
["Hinweise","","","(1) - Innentemperatur: 27°C TK, 19°C FK, Außentemperatur: 35°C TK, 24°C FK","(1) - Innentemperatur: 27°C TK, 19°C FK, Außentemperatur: 35°C TK, 24°C FK","(1) - Innentemperatur: 27°C TK, 19°C FK, Außentemperatur: 35°C TK, 24°C FK","(1) - Innentemperatur: 27°C TK, 19°C FK, Außentemperatur: 35°C TK, 24°C FK","(1) - Innentemperatur: 27°C TK, 19°C FK, Außentemperatur: 35°C TK, 24°C FK"]
["","","","(2) - Innentemperatur: 20°C TK, 15°C FK, Außentemperatur: 7°C TK, 6°C WB.","(2) - Innentemperatur: 20°C TK, 15°C FK, Außentemperatur: 7°C TK, 6°C WB.","(2) - Innentemperatur: 20°C TK, 15°C FK, Außentemperatur: 7°C TK, 6°C WB.","(2) - Innentemperatur: 20°C TK, 15°C FK, Außentemperatur: 7°C TK, 6°C WB.","(2) - Innentemperatur: 20°C TK, 15°C FK, Außentemperatur: 7°C TK, 6°C WB."]