{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":10,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-K1"]
[]
[]
[]
[]
["","","","","","FTXS20K3V1B1","FTXS25K3V1B1","FTXS35K3V1B1","FTXS42K3V1B1","FTXS50K3V1B1"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","0.040, 0.040, 0.040","0.040, 0.040, 0.040","0.026, 0.026, 0.026","0.024, 0.024, 0.024","0.026, 0.026, 0.026"]
["","Heizen","","Nom.","kW","0.040, 0.040, 0.040","0.040, 0.040, 0.040","0.028, 0.028, 0.028","0.030, 0.030, 0.030","0.032, 0.032, 0.032"]
["Gehäuse","Farbe","","","","Weiß","Weiß","Weiß","Weiß","Weiß"]
["Abmessungen","Maßeinheit","","Höhe","mm","289","289","298","298","298"]
["","","","Breite","mm","780","780","900","900","900"]
["","","","Tiefe","mm","215","215","215","215","215"]
["Gewicht","Maßeinheit","","","kg","9","9","12","12","12"]
["Ventilator","Luftstromvolumen","Kühlung","Hoch","m³/min","8.1","9.1","11.2","11.2","11.9"]
["","","Kühlen","Mittel","m³/min","6.7","7.0","8.5","9.1","9.6"]
["","","","Niedrig","m³/min","4.7","5.0","5.8","7.0","7.4"]
["","","","Flüsterbetrieb","m³/min","3.9","3.9","4.1","4.1","4.5"]
["","","Heizen","Hoch","m³/min","10.0","10.0","13.9","13.4","14.3"]
["","","","Mittel","m³/min","8.0","8.0","10.2","10.6","11.3"]
["","","","Niedrig","m³/min","6.0","6.0","6.5","7.8","8.4"]
["","","","Flüsterbetrieb","m³/min","4.3","4.3","4.2","5.2","5.5"]
["Schallleistungspegel","Kühlung","","","dBA","58","58","59","59","60"]
["","Heizen","","","dBA","58","58","59","59","60"]
["Schalldruckpegel","Kühlung","","Hoch","dBA","40","41","45","45","46"]
["","Kühlen","","Mittel","dBA","32","33","37","39","40"]
["","","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dBA","24","25","29","33","34"]
["","","","Flüsterbetrieb","dBA","19","19","19","21","23"]
["","Heizen","","Hoch","dBA","40","41","45","45","47"]
["","","","Mittel","dBA","34","34","39","39","40"]
["","","","Niedrig","dBA","27","27","29","33","34"]
["","","","Flüsterbetrieb","dBA","19","19","19","22","24"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","6.35","6.35","6.35","6.35","6.35"]
["","Gas","","AD","mm","9.50","9.50","9.50","12.70","12.70"]
["","Ableitung","","","","18","18","18","18","18"]
["Regelungssysteme","Infrared remote control","","","","ARC466A6","ARC466A6","ARC466A9","ARC466A9","ARC466A9"]
["Standardzubehör","Installation manual","","","","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","Operation manual","","","","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2","2","2"]
["","Indoor unit fixing screws","","","","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1"]
["Stromversorgung","Bezeichnung","","","","V1","V1","V1","V1","V1"]
["","Phase","","","","1~","1~","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50","50","50"]
["Spannungsversorgung","Spannung","","","V","220-230-240","220-230-240","220-230-240","220-230-240","220-230-240"]
["Hinweise","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V"]
["Standardzubehör","Batteries","","","","","","2","2","2"]