{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":6,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-BW"]
[]
[]
[]
[]
["","","","","","FTXTA30B2V1BW"]
["Schalldruckpegel","Heizen","","Hoch","dB(A)","41"]
["","","","Mittel","dB(A)","31"]
["","","","Flüsterbetrieb","dB(A)","19"]
["","","","Niedrig","dB(A)","24"]
["","Kühlung","","Medium","dB(A)","32"]
["","","","Flüsterbetrieb","dB(A)","20"]
["","","","Niedrig","dB(A)","25"]
["","","","Hoch","dB(A)","43"]
["Standardzubehör","Installationsanleitung","","","","1"]
["","Bedienungsanleitung","","","","1"]
["","Luftfilter","","","","2"]
["","Infrarot-Fernbedienung","","","","1"]
["","Montageplatte für Fernbedienung","","","","1"]
["","Schraubensack","","","","1"]
["","Schraubenabdeckung","","","","2"]
["","Trockenbatterien, Typ AAA","","","","2"]
["","Allgemeine Schutzmaßnahmen","","","","1"]
["Kältemittel","GWP","","","","675.0"]
["Regelungssysteme","Wired remote control","","","","BRC073A4"]
["","Infrared remote control","","","","ARC466A59"]
["Piping connections","Flüssigkeit","","AD","mm","6.35"]
["","Gas","","AD","mm","9.50"]
["","Ableitung","","","","18"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","0.023"]
["","Heizen","","Nom.","kW","0.022"]
["Schallleistungspegel","Kühlung","","","dB(A)","60"]
["","Heizen","","","dB(A)","60"]
["Abmessungen","Gerät","","Breite","mm","798"]
["","","","Tiefe","mm","189"]
["","","","Höhe","mm","295"]
["Gehäuse","Colour","","","","Weiß"]
["Gewicht","Maßeinheit","","","kg","11.5"]
["Ventilator","Luftstromvolumen","Heizen","Hoch","m³/min","11.5"]
["","","","Niedrig","m³/min","6.0"]
["","","","Mittel","m³/min","8.0"]
["","","","Flüsterbetrieb","m³/min","5.1"]
["","","Kühlen","Niedrig","m³/min","5.7"]
["","","","Mittel","m³/min","8.3"]
["","","","Hoch","m³/min","11.9"]
["","","","Flüsterbetrieb","m³/min","4.6"]
["Power supply","Phase","","","","1~"]
["","Frequenz","","","Hz","50"]
["","Bezeichnung","","","","V1"]
["","Spannung","","","V","220-240"]
["Hinweise","","","","","(1) - Kühlen: Innentemperatur: 27°C TK, 19,0°C FK; Außentemp. 35°C TK, 24°C FK; äquivalente Leitungslänge: 5 m"]
["","","","","","(2) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m"]
["","","","","","(3) - Siehe separate Zeichnung für die elektrischen Daten"]