{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":5,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-CB / RXTA-B"]
[]
[]
[]
[]
["","","","","FTXTA30C2V1BB / RXTA30B2V1B"]
["Kühlleistung","Min.","","kW","0.70"]
["","Nom.","","kW","3.00"]
["","Max.","","kW","4.50"]
["Heizleistung","Min.","","kW","0.80"]
["","Nom.","","kW","3.20"]
["","Max.","","kW","6.90"]
["Nominale Effizienz","Jährlicher Energieverbrauch","","kWh","357"]
["","COP","","","4.87"]
["","EER","","","4.20"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","A"]
["","","Heizen","","A"]
["Hinweise","","","","(1) - Nennkühlleistungen basieren auf: Innentemp.: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m."]
["","","","","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m."]
["","","","","(3) - Siehe separate Zeichnung für die elektrischen Daten"]
["","","","","(4) - Siehe separate Zeichnung für den Betriebsbereich"]