{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":6,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-CB"]
[]
[]
[]
[]
["","","","","","FTXTA30C2V1BB"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","0.023"]
["","Heizen","","Nom.","kW","0.022"]
["Gehäuse","Farbe","","","","Schwarz"]
["Abmessungen","Maßeinheit","","Höhe","mm","295"]
["","","","Breite","mm","798"]
["","","","Tiefe","mm","189"]
["Gewicht","Maßeinheit","","","kg","12"]
["Ventilator","Luftstromvolumen","Kühlung","Hoch","m³/min","13.1"]
["","","Kühlen","Mittel","m³/min","9"]
["","","","Niedrig","m³/min","6"]
["","","","Flüsterbetrieb","m³/min","4.9"]
["","","Heizen","Hoch","m³/min","12.3"]
["","","","Mittel","m³/min","8.2"]
["","","","Niedrig","m³/min","5.8"]
["","","","Flüsterbetrieb","m³/min","5"]
["Schallleistungspegel","Kühlung","","","dBA","60"]
["","Heizen","","","dBA","60"]
["Schalldruckpegel","Kühlung","","Hoch","dBA","43"]
["","Kühlen","","Mittel","dBA","32"]
["","","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dBA","25"]
["","","","Flüsterbetrieb","dBA","20"]
["","Heizen","","Hoch","dBA","41"]
["","","","Mittel","dBA","31"]
["","","","Niedrig","dBA","24"]
["","","","Flüsterbetrieb","dBA","19"]
["Kältemittel","GWP","","","","675"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","6.35"]
["","Gas","","AD","mm","9.5"]
["","Ableitung","","","","18"]
["Regelungssysteme","Infrared remote control","","","","ARC466A84"]
["Regelungssysteme","Verkabelte Fernbedienung","","","","BRC073A4"]
["Standardzubehör","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","Screw cover","","","","2"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","1"]
["","Silver particle filter","","","","1"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","1"]
["Stromversorgung","Phase","","","","1~"]
["","Frequenz","","","Hz","50"]
["Spannungsversorgung","Spannung","","","V","220-240"]