{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":6,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-DY"]
[]
[]
[]
[]
["","","","","","FTXTA30D2V1BY"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","0.023"]
["","Heizen","","Nom.","kW","0.022"]
["Gehäuse","Farbe","","","","Casing: Black, Panel: Dark wood"]
["Abmessungen","Maßeinheit","","Höhe","mm","295"]
["","","","Breite","mm","798"]
["","","","Tiefe","mm","189"]
["Gewicht","Maßeinheit","","","kg","12"]
["Ventilator","Luftstromvolumen","Kühlung","Hoch","m³/min","13.1"]
["","","Kühlen","Mittel","m³/min","9.0"]
["","","","Niedrig","m³/min","6.0"]
["","","","Flüsterbetrieb","m³/min","4.9"]
["","","Heizen","Hoch","m³/min","12.3"]
["","","","Mittel","m³/min","8.2"]
["","","","Niedrig","m³/min","5.8"]
["","","","Flüsterbetrieb","m³/min","5.0"]
["Schallleistungspegel","Kühlung","","","dB(A)","60"]
["","Heizen","","","dB(A)","60"]
["Schalldruckpegel","Kühlung","","Hoch","dB(A)","43"]
["","Kühlen","","Schalldruckpegel-=-Kühlen-=-Mittel-=-dB(A)","dB(A)","32"]
["","","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dB(A)","25"]
["","","","Flüsterbetrieb","dB(A)","20"]
["","Heizen","","Hoch","dB(A)","41"]
["","","","Schalldruckpegel-=-Heizen-=-Mittel-=-dB(A)","dB(A)","31"]
["","","","Niedrig","dB(A)","24"]
["","","","Flüsterbetrieb","dB(A)","19"]
["Kältemittel","GWP","","","","675.0"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","6.35"]
["","Gas","","AD","mm","9.50"]
["","Ableitung","","","","18"]
["Regelungssysteme","Infrarot-Fernbedienung","","","","ARC466A95"]
["","Verkabelte Fernbedienung","","","","BRC073A1"]
["Standardzubehör","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","Screw cover","","","","2"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","1"]
["","Silver particle filter","","","","1"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","1"]
["Energieeffizienzbereich","","","","","A+++ ~ D"]
["Stromversorgung","Phase","","","","1~"]
["","Frequenz","","","Hz","50"]
["Spannungsversorgung","Spannung","","","V","220-240"]
["Hinweise","","","","","(1) - Kühlen: Innentemperatur: 27°C TK, 19°C FK, Außentemp. 35°C TK, 24°C FK; äquivalente Leitungslänge: 5 m"]
["","","","","","(2) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m"]
["","","","","","(3) - Siehe separate Zeichnung für die elektrischen Daten"]