{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":7,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-M"]
[]
[]
[]
[]
["","","","","","FTXTM30M2V1B","FTXTM40M2V1B"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","0.032","0.037"]
["","Heizen","","Nom.","kW","0.037","0.04"]
["Gehäuse","Farbe","","","","Weiß","Weiß"]
["Abmessungen","Maßeinheit","","Höhe","mm","294","300"]
["","","","Breite","mm","811","1040"]
["","","","Tiefe","mm","272","295"]
["Gewicht","Maßeinheit","","","kg","10","14.5"]
["Ventilator","Luftstromvolumen","Kühlung","Hoch","m³/min","11.7","15.5"]
["","","Kühlen","Mittel","m³/min","8","9.2"]
["","","","Niedrig","m³/min","6.3","5.7"]
["","","","Flüsterbetrieb","m³/min","5.2","4.6"]
["","","Heizen","Hoch","m³/min","12.2","17.7"]
["","","","Mittel","m³/min","7.5","11"]
["","","","Niedrig","m³/min","5.1","7.5"]
["","","","Flüsterbetrieb","m³/min","4.1","6.3"]
["Schallleistungspegel","Kühlung","","","dBA","60","60"]
["","Heizen","","","dBA","61","61"]
["Schalldruckpegel","Kühlung","","Hoch","dBA","45","46"]
["","Kühlen","","Mittel","dBA","33","32"]
["","","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dBA","25","24"]
["","","","Flüsterbetrieb","dBA","21","20"]
["","Heizen","","Hoch","dBA","45","46"]
["","","","Mittel","dBA","31","31"]
["","","","Niedrig","dBA","22","22"]
["","","","Flüsterbetrieb","dBA","19","19"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","6.35","6.35"]
["","Gas","","AD","mm","9.5","9.5"]
["","Ableitung","","","","16 (Innendurchmesser des Anschlussschlauchs)","16 (Innendurchmesser des Anschlussschlauchs)"]
["Regelungssysteme","Infrarot-Fernbedienung","","","","ARC466A55","ARC466A55"]
["","Verkabelte Fernbedienung","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Stromversorgung","Bezeichnung","","","","V1","V1"]
["","Phase","","","","1~","1~"]
["","Frequenz","","","Hz","50","50"]
["Spannungsversorgung","Spannung","","","V","220-240","220-240"]