{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":94,"n_cols":7,"rows_kept":94,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-R"]
[]
[]
[]
[]
["","","","","","FTXTM30R2V1B","FTXTM40R2V1B"]
["Schalldruckpegel","Heizen","","Hoch","dBA","45.0"]
["","","","Mittel","dBA","31.0"]
["","","","Flüsterbetrieb","dBA","19.0"]
["","","","Niedrig","dBA","22.0"]
["","Kühlung","","Mittel","dBA","33.0"]
["","","","Flüsterbetrieb","dBA","21.0"]
["","","","Niedrig","dBA","25.0"]
["","","","Hoch","dBA","45.0"]
["Standardzubehör","Installationsanleitung","","","","1"]
["","Bedienungsanleitung","","","","1"]
["","Infrarotfernbedienung","","","","1"]
["","Trockenbatterien, Typ AAA","","","","2"]
["","Fernbedienungshalterung","","","","1"]
["","Montageplatte","","","","1"]
["","Befestigungsschrauben für Hauptgerät","","","","2"]
["","Silber-Partikelfilter","","","","1"]
["Regelungssysteme","Verkabelte Fernbedienung","","","","BRC073A1"]
["","Infrared remote control","","","","ARC466A75"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","6.35"]
["","Gas","","AD","mm","9.50"]
["","Ableitung","","","","18"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","0.035"]
["","Heizen","","Nom.","kW","0.039"]
["Schallleistungspegel","Kühlung","","","dBA","60.0"]
["","Heizen","","","dBA","61.0"]
["Abmessungen","Maßeinheit","","Breite","mm","778"]
["","","","Tiefe","mm","272"]
["","","","Höhe","mm","295"]
["Gehäuse","Farbe","","","","Weiß"]
["Gewicht","Maßeinheit","","","kg","10.0"]
["Ventilator","Luftstromvolumen","Heizen","Hoch","m³/min","12.5"]
["","","","Niedrig","m³/min","4.9"]
["","","","Mittel","m³/min","7.5"]
["","","","Flüsterbetrieb","m³/min","4.0"]
["","","Kühlung","Niedrig","m³/min","5.3"]
["","","","Mittel","m³/min","7.8"]
["","","","Hoch","m³/min","12.2"]
["","","","Flüsterbetrieb","m³/min","4.1"]
["Power supply","Phase","","","","1~"]
["","Frequenz","","","Hz","50"]
["","Bezeichnung","","","","V1"]
["","Spannung","","","V","220-240"]
["Hinweise","","","","","(1) - Kühlen: Innentemperatur: 27°C TK, 19,0°C FK; Außentemp. 35°C TK, 24°C FK; äquivalente Leitungslänge: 5 m"]
["","","","","","(2) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m"]
["","","","","","(3) - Siehe separate Zeichnungen für die elektrischen Daten"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","","0.053"]
["","Heizen","","Nom.","kW","","0.06"]
["Gehäuse","Farbe","","","","","Weiß"]
["Abmessungen","Maßeinheit","","Höhe","mm","","299"]
["","","","Breite","mm","","998"]
["","","","Tiefe","mm","","292"]
["Gewicht","Maßeinheit","","","kg","","14.5"]
["Ventilator","Luftstromvolumen","Kühlung","Hoch","m³/min","","15.4"]
["","","Kühlen","Mittel","m³/min","","9.5"]
["","","","Niedrig","m³/min","","5.8"]
["","","","Flüsterbetrieb","m³/min","","4.6"]
["","","Heizen","Hoch","m³/min","","17.5"]
["","","","Mittel","m³/min","","10.5"]
["","","","Niedrig","m³/min","","7.1"]
["","","","Flüsterbetrieb","m³/min","","5.9"]
["Schallleistungspegel","Kühlung","","","dBA","","60"]
["","Heizen","","","dBA","","61"]
["Schalldruckpegel","Kühlung","","Hoch","dBA","","46"]
["","Kühlen","","Mittel","dBA","","32"]
["","","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dBA","","24"]
["","","","Flüsterbetrieb","dBA","","20"]
["","Heizen","","Hoch","dBA","","46"]
["","","","Mittel","dBA","","31"]
["","","","Niedrig","dBA","","22"]
["","","","Flüsterbetrieb","dBA","","19"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","","6.35"]
["","Gas","","AD","mm","","9.5"]
["","Ableitung","","","","","18"]
["Regelungssysteme","Infrared remote control","","","","","ARC466A75"]
["Regelungssysteme","Verkabelte Fernbedienung","","","","","BRC073A1"]
["Standardzubehör","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","1"]
["","Silver particle filter","","","","","1"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["Stromversorgung","Bezeichnung","","","","","V1"]
["","Phase","","","","","1~"]
["","Frequenz","","","Hz","","50"]
["Spannungsversorgung","Spannung","","","V","","220-240"]