{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-S / RXTM-A"]
[]
[]
[]
[]
["","","","","FTXTM30S2V1B / RXTM30A2V1B","FTXTM40S2V1B / RXTM40A2V1B"]
["Kühlleistung","Min.","","kW","1.2","1.2"]
["","Nom.","","kW","3","4"]
["","Max.","","kW","4.6","5.2"]
["Heizleistung","Min.","","kW","0.8","0.9"]
["","Nom.","","kW","3.2","4"]
["","Max.","","kW","7.4","8.8"]
["Nominale Effizienz","EER","","","5.13","4.71"]
["","COP","","","5.2","5.51"]
["","Jährlicher Energieverbrauch","","kWh","292","425"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","A","A"]
["","","Heizen","","A","A"]
["Raumkühlen","Energieeffizienzklasse","","","A+++","A+++"]
["","Leistung","Pdesign","kW","3","4"]
["","SEER","","","8.65","8.93"]
["","Jährlicher Energieverbrauch","","kWh/a","121","157"]
["Raumheizen (Durchschnittliches Klima)","Energieeffizienzklasse","","","A+++","A+++"]
["","Leistung","Pdesign","kW","3","3.8"]
["","SCOP/A","","","5.2","5.5"]
["","Raumheizen (Durchschnittliches Klima)-=-Heizleistung&nbsp;Pdh bei&nbsp;-10°-=-kW","","kW","3","3.8"]
["","Jährlicher Energieverbrauch","","kWh/a","807","967"]
["Hinweise","","","","(1) - Siehe separate Zeichnung für die elektrischen Daten","(1) - Siehe separate Zeichnung für die elektrischen Daten"]
["","","","","(2) - Siehe separate Zeichnung für den Betriebsbereich","(2) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","(3) - Nennkühlleistungen basieren auf: Innentemp.: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m.","(3) - Nennkühlleistungen basieren auf: Innentemp.: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m."]
["","","","","(4) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m.","(4) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m."]