{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-A"]
[]
[]
[]
[]
["","","","","","FTXTP25A5V1B","FTXTP35A5V1B"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","0.032","0.032"]
["","Heizen","","Nom.","kW","0.032","0.032"]
["Gehäuse","Farbe","","","","Weiß","Weiß"]
["Abmessungen","Maßeinheit","","Höhe","mm","286","286"]
["","","","Breite","mm","770","770"]
["","","","Tiefe","mm","225","225"]
["Gewicht","Maßeinheit","","","kg","9","9"]
["Ventilator","Luftstromvolumen","Kühlung","Hoch","m³/min","11","11"]
["","","Kühlen","Mittel","m³/min","7.9","7.9"]
["","","","Niedrig","m³/min","5","5"]
["","","","Flüsterbetrieb","m³/min","3.7","3.7"]
["","","Heizen","Hoch","m³/min","10.5","10.5"]
["","","","Mittel","m³/min","9","9"]
["","","","Niedrig","m³/min","5.5","5.5"]
["","","","Flüsterbetrieb","m³/min","4.4","4.4"]
["Schallleistungspegel","Kühlung","","","dBA","58","58"]
["","Heizen","","","dBA","58","58"]
["Schalldruckpegel","Kühlung","","Hoch","dBA","43","43"]
["","Kühlen","","Mittel","dBA","35","35"]
["","","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dBA","26","26"]
["","","","Flüsterbetrieb","dBA","21","21"]
["","Heizen","","Hoch","dBA","43","43"]
["","","","Mittel","dBA","35","35"]
["","","","Niedrig","dBA","26","26"]
["","","","Flüsterbetrieb","dBA","21","21"]
["Kältemittel","GWP","","","","675","675"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","6.35","6.35"]
["","Gas","","AD","mm","9.5","9.5"]
["","Ableitung","","","","18","18"]
["Regelungssysteme","Infrared remote control","","","","ARC480A78","ARC480A78"]
["Standardzubehör","FTXTP25A5V1B","","","","1"]
["","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","Screw cover","","","","2","2"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Screw bag","","","","1","1"]
["Stromversorgung","Bezeichnung","","","","V1","V1"]
["","Phase","","","","1~","1~"]
["","Frequenz","","","Hz","50","50"]
["Spannungsversorgung","Spannung","","","V","220-240","220-240"]
["Hinweise","","","","","(1) - Kühlen: Innentemperatur: 27°C TK, 19°C FK, Außentemp. 35°C TK, 24°C FK; äquivalente Leitungslänge: 5 m","(1) - Kühlen: Innentemperatur: 27°C TK, 19°C FK, Außentemp. 35°C TK, 24°C FK; äquivalente Leitungslänge: 5 m"]
["","","","","","(2) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m","(2) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m"]
["","","","","","(3) - Siehe separate Zeichnung für die elektrischen Daten","(3) - Siehe separate Zeichnung für die elektrischen Daten"]
["Standardzubehör","FTXTP35A5V1B","","","","","1"]