{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":83,"n_cols":7,"rows_kept":83,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-K"]
[]
[]
[]
[]
["","","","","","FTXTP25K3V1B","FTXTP35K3V1B"]
["Schalldruckpegel","Heizen","","Hoch","dBA","43"]
["","","","Mittel","dBA","35"]
["","","","Flüsterbetrieb","dBA","21"]
["","","","Niedrig","dBA","26"]
["","Kühlung","","Medium","dBA","35"]
["","","","Flüsterbetrieb","dBA","21"]
["","","","Niedrig","dBA","26"]
["","","","Hoch","dBA","43"]
["Standardzubehör","Installationsanleitung","","","","1"]
["","Bedienungsanleitung","","","","1"]
["","Infrarotfernbedienung","","","","1"]
["","Trockenbatterien, Typ AAA","","","","2"]
["","Fernbedienungshalterung","","","","1"]
["","Montageplatte","","","","1"]
["","Geruchsfilter mit Titanapatit","","","","2"]
["","Befestigungsschrauben für Hauptgerät","","","","2"]
["Regelungssysteme","Wired remote control","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","ARC480A11"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","6.35"]
["","Gas","","AD","mm","9.50"]
["","Drain","","","","16 (Innendurchmesser des Anschlussschlauchs)"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","0.030"]
["","Heizen","","Nom.","kW","0.035"]
["Schallleistungspegel","Kühlung","","","dBA","58"]
["","Heizen","","","dBA","58"]
["Abmessungen","Maßeinheit","","Breite","mm","770"]
["","","","Tiefe","mm","225"]
["","","","Höhe","mm","285"]
["Gehäuse","Colour","","","","Weiß"]
["Gewicht","Maßeinheit","","","kg","9.0"]
["Power supply","Phase","","","","1~"]
["","Frequenz","","","Hz","50"]
["","Bezeichnung","","","","V1"]
["","Spannung","","","V","220-240"]
["Hinweise","","","","","(1) - Siehe separate Zeichnung für die elektrischen Daten"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","","0.03"]
["","Heizen","","Nom.","kW","","0.035"]
["Gehäuse","Farbe","","","","","Weiß"]
["Abmessungen","Maßeinheit","","Höhe","mm","","285"]
["","","","Breite","mm","","770"]
["","","","Tiefe","mm","","225"]
["Gewicht","Maßeinheit","","","kg","","9"]
["Ventilator","Luftstromvolumen","Kühlung","Hoch","m³/min","","11.4"]
["","","Kühlen","Mittel","m³/min","","8.2"]
["","","","Niedrig","m³/min","","5.4"]
["","","","Flüsterbetrieb","m³/min","","4.3"]
["","","Heizen","Hoch","m³/min","","10.8"]
["","","","Mittel","m³/min","","7.8"]
["","","","Niedrig","m³/min","","5.8"]
["","","","Flüsterbetrieb","m³/min","","4.9"]
["Schallleistungspegel","Kühlung","","","dBA","","58"]
["","Heizen","","","dBA","","58"]
["Schalldruckpegel","Kühlung","","Hoch","dBA","","43"]
["","Kühlen","","Mittel","dBA","","35"]
["","","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dBA","","26"]
["","","","Flüsterbetrieb","dBA","","21"]
["","Heizen","","Hoch","dBA","","43"]
["","","","Mittel","dBA","","35"]
["","","","Niedrig","dBA","","26"]
["","","","Flüsterbetrieb","dBA","","21"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","","6.35"]
["","Gas","","AD","mm","","9.5"]
["","Ableitung","","","","","16 (Innendurchmesser des Anschlussschlauchs)"]
["Regelungssysteme","Infrared remote control","","","","","ARC480A11"]
["Regelungssysteme","Verkabelte Fernbedienung","","","","","BRC944B2, BRC073A1"]
["Standardzubehör","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","2"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["Stromversorgung","Bezeichnung","","","","","V1"]
["","Phase","","","","","1~"]
["","Frequenz","","","Hz","","50"]
["Spannungsversorgung","Spannung","","","V","","220-240"]