{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":8,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXZ-N"]
[]
[]
[]
[]
["","","","","","FTXZ25NV1B","FTXZ35NV1B","FTXZ50NV1B"]
["Schalldruckpegel","Heizen","","Hoch","dB(A)","39","42","44"]
["","","","Flüsterbetrieb","dB(A)","19","19","24"]
["","","","Niedrig","dB(A)","28","29","31"]
["","Kühlung","","Flüsterbetrieb","dB(A)","19","19","23"]
["","","","Niedrig","dB(A)","26","27","30"]
["","","","Hoch","dB(A)","38","42","47"]
["","","","Nom.","dB(A)","35","36","38"]
["","Kühlung","","Nom.","dB(A)","33","35","38"]
["Standardzubehör","Photokatalytische Luftreinigung und geruchsbindender Filter","","","","1","1","1"]
["","Infrarotfernbedienung","","","","1","1","1"]
["","Trockenbatterien","","","","2","2","2"]
["","Fernbedienungshalterung","","","","1","1","1"]
["","Befestigungsschrauben für Hauptgerät","","","","3","3","3"]
["","Montageplatte","","","","1","1","1"]
["Regelungssysteme","Infrared remote control","","","","ARC477A1","ARC477A1","ARC477A1"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","6.35","6.35","6.35"]
["","Gas","","AD","mm","9.5","9.5","9.5"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","0.030","0.030","0.030"]
["","Heizen","","Nom.","kW","0.030","0.030","0.030"]
["Sound power level","Kühlung","","","dB(A)","54","57","60"]
["","Heizen","","","dB(A)","56","57","59"]
["Abmessungen","Maßeinheit","","Breite","mm","798","798","798"]
["","","","Tiefe","mm","372","372","372"]
["","","","Höhe","mm","295","295","295"]
["Gehäuse","Colour","","","","Weiß","Weiß","Weiß"]
["Gewicht","Maßeinheit","","","kg","15","15","15"]
["Ventilator","Luftstromvolumen","Heizen","Hoch","m³/min","11.7","13.3","14.4"]
["","","","Niedrig","m³/min","6.7","6.9","7.7"]
["","","","Flüsterbetrieb","m³/min","4.8","4.8","5.9"]
["","","Kühlung","Niedrig","m³/min","5.3","5.6","6.6"]
["","","","Hoch","m³/min","10.7","12.1","15.0"]
["","","","Flüsterbetrieb","m³/min","4.0","4.0","4.6"]
["","","","Nom.","m³/min","8.6","9.2","10.7"]
["","","Kühlung","Nom.","m³/min","7.5","8.4","9.2"]
["Power supply","Phase","","","","1~","1~","1~"]
["","Bezeichnung","","","","V1","V1","V1"]
["","Frequenz","","","Hz","50","50","50"]
["","Spannung","","","V","220-240","220-240","220-240"]
["Hinweise","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V"]
["","","","","","(4) - Vorderseite des Wärmetauschers","(4) - Vorderseite des Wärmetauschers","(4) - Vorderseite des Wärmetauschers"]
["","","","","","(5) - Rückseite des Wärmetauschers","(5) - Rückseite des Wärmetauschers","(5) - Rückseite des Wärmetauschers"]