{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":82,"n_cols":11,"rows_kept":82,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A"]
[]
[]
[]
[]
["","","","","","FUA71AVEB9","FUA100AVEB9","FUA125AVEB9","FUA71AVEB (Archived)","FUA100AVEB (Archived)","FUA125AVEB (Archived)"]
["Schalldruckpegel","Heizen","","Hoch","dB(A)","","","","41","46","47"]
["","","","Mittel","dB(A)","","","","38","42","43"]
["","","","Niedrig","dB(A)","","","","35","39","40"]
["","Kühlung","","Medium","dB(A)","","","","38","42","43"]
["","","","Niedrig","dB(A)","","","","35","39","40"]
["","","","Hoch","dB(A)","","","","41","46","47"]
["Standardzubehör","Bedienungsanleitung","","","","","","","1","1","1"]
["","Installationsanleitung","","","","","","","1","1","1"]
["","Kondensatschlauch","","","","","","","1","1","1"]
["","Wärmeisolierrohr","","","","","","","3","3","3"]
["","Kabelbinder","","","","","","","10","10","10"]
["","Schlauchband","","","","","","","1","1","1"]
["","Dichtungsmaterial","","","","","","","4","4","4"]
["","Unterlegscheibe für Befestigungsplatte","","","","","","","1","1","1"]
["","Ableitungspunkt","","","","","","","1","1","1"]
["","Vliesstoff","","","","","","","1","1","1"]
["","Unterlegscheibe","","","","","","","8","8","8"]
["","Befestigungsschraube für Kondensatschlauch","","","","","","","5","5","5"]
["Regelungssysteme","Verkabelte Fernbedienung","","","","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Kühlleistung","Gesamtleistung","","Nom.","kW","","","","","","12.1"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","","","","9.52","9.52","9.52"]
["","Gas","","AD","mm","","","","15.9","15.9","15.9"]
["","Ableitung","","","","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Sound power level","Kühlung","","","dB(A)","","","","59","64","65"]
["","Heizen","","","dB(A)","","","","59","64"]
["Abmessungen","Maßeinheit","","Breite","mm","","","","950","950","950"]
["","","","Tiefe","mm","","","","950","950","950"]
["","","","Höhe","mm","","","","198","198","198"]
["Gehäuse","Material","","","","","","","Kunststoff","Kunststoff","Kunststoff"]
["","Farbe","","","","","","","Reinweiß","Reinweiß","Reinweiß"]
["Gewicht","Maßeinheit","","","kg","","","","25.0","26.0","26"]
["Ventilator","Luftstromvolumen","Heizen","Hoch","m³/min","","","","23.0","31.0","32.5"]
["","","","Mittel","m³/min","","","","19.5","25.5","26.5"]
["","","","Niedrig","m³/min","","","","16.0","20.0","20.5"]
["","","Kühlung","Niedrig","m³/min","","","","16.0","20.0","20.5"]
["","","","Mittel","m³/min","","","","19.5","25.5","26.5"]
["","","","Hoch","m³/min","","","","23.0","31.0","32.5"]
["Entleerungshöhe","mm","","","","","","","600","600","600"]
["Heizleistung","Gesamtleistung","","Nom.","kW","","","","","","13.5"]
["Gehäuse","Farbe","","","","Reinweiß","Reinweiß","Reinweiß"]
["","Material","","","","Kunststoff","Kunststoff","Kunststoff"]
["Abmessungen","Maßeinheit","","Höhe","mm","198","198","198"]
["","","","Breite","mm","950","950","950"]
["","","","Tiefe","mm","950","950","950"]
["Gewicht","Maßeinheit","","","kg","25.0","26.0","26.0"]
["Ventilator","Luftstromvolumen","Kühlung","Hoch","m³/min","23.0","31.0","32.5"]
["","","Kühlen","Mittel","m³/min","19.5","25.5","26.5"]
["","","","Niedrig","m³/min","16.0","20.0","20.5"]
["","","Heizen","Hoch","m³/min","23.0","31.0","32.5"]
["","","","Mittel","m³/min","19.5","25.5","26.5"]
["","","","Niedrig","m³/min","16.0","20.0","20.5"]
["Schallleistungspegel","Kühlung","","","dB(A)","59","64","65"]
["Schalldruckpegel","Kühlung","","Hoch","dB(A)","41","46","47"]
["","Kühlen","","Mittel","dB(A)","38","42","43"]
["","","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dB(A)","35","39","40"]
["","Heizen","","Hoch","dB(A)","41","46","47"]
["","","","Mittel","dB(A)","38","42","43"]
["","","","Niedrig","dB(A)","35","39","40"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","9.52","9.52","9.52"]
["","Gas","","AD","mm","15.9","15.9","15.9"]
["","Ableitung","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Entleerungshöhe","mm","","","","600","600","600"]
["Standardzubehör","Installation manual","","","","1","1","1"]
["","Thermal insulation tube","","","","3","3","3"]
["","Non woven fabric","","","","1","1","1"]
["","Drain joint","","","","1","1","1"]
["","Hose band","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Drain hose","","","","1","1","1"]
["","Fixing screw for drain hose","","","","5","5","5"]
["","Sealing material","","","","4","4","4"]
["","Tie-wraps","","","","10","10","10"]
["","Washer","","","","8","8","8"]
["","Washer fixing plate","","","","1","1","1"]
["Kühlleistung","Gesamtleistung","","Nom.","kW","","","12.10"]
["Heizleistung","Gesamtleistung","","Nom.","kW","","","13.5"]