{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":8,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUQ-C / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FUQ71CVEB / RZQG71L9V1B","FUQ71CVEB / FUQ71CVEB / RZQG100L9V1B","FUQ71CVEB / FUQ71CVEB / RZQG125L9V1B","FUQ125CVEB / RZQG125L9V1B"]
["Kühlleistung","Nom.","","kW","6.8","","","12.0"]
["Raumkühlen","SEER","","","6.42","5.10","5.10","5.61"]
["","Jährlicher Energieverbrauch","","kWh/a","371","652","824","749"]
["","Leistung","Pdesign","kW","6.80","9.50","12.00","12.00"]
["","Energieeffizienzklasse","","","A++","B","B","A+"]
["Raumheizen (Durchschnittliches Klima)","Leistung","Pdesign","kW","7.60","11.30","12.71","14.13"]
["","SCOP/A","","","4.20","3.80","3.80","4.44"]
["","Energieeffizienzklasse","","","A+","A","A","A+"]
["","Jährlicher Energieverbrauch","","kWh/a","2,534","4,164","4,683","4,456"]
["Nominale Effizienz","Jährlicher Energieverbrauch","","kWh","840","","","1,770"]
["","EER","","","4.05","","","3.39"]
["","COP","","","4.08","","","3.42"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","A","","","A"]
["","","Heizen","","A","","","B"]
["Heizleistung","Nom.","","kW","7.5","","","13.5"]
["Hinweise","","","","(1) - Jährlicher Energieverbrauch gemäß der Energieetikett-Richtlinie 2002/31/EC","","","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU"]
["","","","","(2) - SEER und SCOP gemäß EN 14825","","","(2) - Nominale Effizienz: Kühlen bei 35 °C/27 °C Nennlast, Heizen bei 7 °C/20 °C Nennlast"]