{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":7,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUQ-C"]
[]
[]
[]
[]
["","","","","FUQ71CVEB","FUQ100CVEB","FUQ125CVEB"]
["Schalldruckpegel","Heizen","Hoch","dBA","41","46","47"]
["","","Nom.","dBA","38","42","43"]
["","","Niedrig","dBA","35","39","40"]
["","Kühlung","Niedrig","dBA","35","39","40"]
["","","Hoch","dBA","41","46","47"]
["","","Nom.","dBA","38","42","43"]
["Standardzubehör","Installationsanleitung","","","Installationsanleitung","Installationsanleitung","Installationsanleitung"]
["","Bedienungsanleitung","","","Bedienungsanleitung","Bedienungsanleitung","Bedienungsanleitung"]
["","Konformitätserklärung","","","Konformitätserklärung","Konformitätserklärung","Konformitätserklärung"]
["","Kondensatschlauch","","","Kondensatschlauch","Kondensatschlauch","Kondensatschlauch"]
["","Klemmblech","","","Klemmblech","Klemmblech","Klemmblech"]
["","Unterlegscheibe für Aufhängung","","","Unterlegscheibe für Aufhängung","Unterlegscheibe für Aufhängung","Unterlegscheibe für Aufhängung"]
["","Klemmen","","","Klemmen","Klemmen","Klemmen"]
["","Unterlegscheibenschelle","","","Unterlegscheibenschelle","Unterlegscheibenschelle","Unterlegscheibenschelle"]
["","Verbindungsstückisolierung und Dichtungsmaterial","","","Verbindungsstückisolierung und Dichtungsmaterial","Verbindungsstückisolierung und Dichtungsmaterial","Verbindungsstückisolierung und Dichtungsmaterial"]
["","Kniestück","","","Kniestück","Kniestück","Kniestück"]
["","Installationsmuster","","","Installationsmuster","Installationsmuster","Installationsmuster"]
["","Sperrmaterial","","","Sperrmaterial","Sperrmaterial","Sperrmaterial"]
["","L-förmige Leitung","","","L-förmige Leitung","L-förmige Leitung","L-förmige Leitung"]
["","Schrauben","","","Schrauben","Schrauben","Schrauben"]
["","Vliesstoff","","","Vliesstoff","Vliesstoff","Vliesstoff"]
["Regelungssysteme","Wired remote control","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["","Infrared remote control","","","BRC7C58","BRC7C58","BRC7C58"]
["Rohrleitungsanschlüsse","Flüssigkeit","AD","mm","9.52","9.52","9.52"]
["","Gas","AD","mm","15.9","15.9","15.9"]
["","Ableitung","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Sound power level","Kühlung","","dBA","59","64","65"]
["","Heizen","","dBA","59","64","65"]
["Abmessungen","Maßeinheit","Breite","mm","950","950","950"]
["","","Tiefe","mm","950","950","950"]
["","","Höhe","mm","198","198","198"]
["Gehäuse","Material","","","Kunststoff","Kunststoff","Kunststoff"]
["","Farbe","","","Reinweiß","Reinweiß","Reinweiß"]
["Gewicht","Maßeinheit","","kg","25","26","26"]
["Entleerungshöhe","mm","","","600","600","600"]
["Power supply","Phase","","","1~","1~","1~"]
["","Frequenz","","Hz","50/60","50/60","50/60"]
["","Bezeichnung","","","VE","VE","VE"]
["","Spannung","","V","220-240/220","220-240/220","220-240/220"]