{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":8,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVA-A / RZASG-MY1"]
[]
[]
[]
[]
["","","","","FVA100AMVEB / RZASG100M7Y1B","FVA125AMVEB / RZASG125M7Y1B","FVA140AMVEB / RZASG140M7Y1B","FVA71AMVEB / FVA71AMVEB / RZASG140M7Y1B"]
["Kühlleistung","Nom.","","kW","","12.1 (1)","13.4 (1)"]
["Raumkühlen","Jährlicher Energieverbrauch","","kWh/a","","1,314","1,428"]
["","Leistung","Pdesign","kW","","12.1","13.4"]
["Raumheizen (Durchschnittliches Klima)","Leistung","Pdesign","kW","","6.00","7.80"]
["","Jährlicher Energieverbrauch","","kWh/a","","2,308","2,866"]
["Heizleistung","Nom.","","kW","","13.5 (2)","15.5 (2)"]
["Kühlleistung","Nom.","","kW","9.5","","","13.4"]
["Heizleistung","Nom.","","kW","10.8","","","15.5"]
["Raumkühlen","Energieeffizienzklasse","","","A+"]
["","Leistung","Pdesign","kW","9.5","","","13.4"]
["","SEER","","","5.72","","","7.71"]
["","Jährlicher Energieverbrauch","","kWh/a","581","","","1043"]
["Raumheizen (Durchschnittliches Klima)","Energieeffizienzklasse","","","A"]
["","Leistung","Pdesign","kW","6","","","7.80"]
["","SCOP/A","","","3.83","","","4.43"]
["","Jährlicher Energieverbrauch","","kWh/a","2193","","","2467"]
["Raumkühlen","SEER","","","","5.52","5.63"]
["Raumheizen (Durchschnittliches Klima)","SCOP/A","","","","3.64","3.81"]
["Hinweise","","","","","(1) - Nennkühlleistungen basieren auf: Innentemp.: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m.","(1) - Nennkühlleistungen basieren auf: Innentemp.: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m.","(1) - Nennkühlleistungen basieren auf: Innentemp.: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m."]
["","","","","","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m.","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m.","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m."]
["","","","","","(3) - Siehe separate Zeichnung für den Betriebsbereich","(3) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","","(4) - Siehe separate Zeichnung für die elektrischen Daten","(4) - Siehe separate Zeichnung für die elektrischen Daten"]