{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":9,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVA-A"]
[]
[]
[]
[]
["","","","","","FVA71AMVEB","FVA100AMVEB","FVA125AMVEB","FVA140AMVEB"]
["Kühlleistung","Gesamtleistung","","Nom.","kW","","","12.10","13.40"]
["Heizleistung","Gesamtleistung","","Nom.","kW","","","13.5","15.5"]
["Gehäuse","Farbe","","","","Reinweiß","Reinweiß","Reinweiß","Reinweiß"]
["Abmessungen","Maßeinheit","","Höhe","mm","1850","1850","1850","1850"]
["","","","Breite","mm","600","600","600","600"]
["","","","Tiefe","mm","270","350","350","350"]
["Gewicht","Maßeinheit","","","kg","42","50","50","50"]
["Ventilator","Luftstromvolumen","Kühlung","Hoch","m³/min","18","28","28","30"]
["","","Kühlen","Mittel","m³/min","16","25","26","28"]
["","","","Niedrig","m³/min","14","22","24","26"]
["","","Heizen","Hoch","m³/min","18","28","28","30"]
["","","","Mittel","m³/min","16","25","26","28"]
["","","","Niedrig","m³/min","14","22","24","26"]
["Schallleistungspegel","Kühlung","","","dB(A)","55","62","63","65"]
["Schalldruckpegel","Kühlung","","Hoch","dB(A)","43","50","51","53"]
["","Kühlen","","Mittel","dB(A)","41","","48","51"]
["","","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dB(A)","38","44","46","48"]
["","Heizen","","Hoch","dB(A)","43","50","51","53"]
["","","","Mittel","dB(A)","38","","46","48"]
["","","","Schalldruckpegel-=-Heizen-=-Nom.-=-dBA","dB(A)","41","","48","51"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","9.52","9.52","9.52","9.52"]
["","Gas","","AD","mm","15.9","15.9","15.9","15.9"]
["","Ableitung","","","","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26"]
["Regelungssysteme","Verkabelte Fernbedienung","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Standardzubehör","Installation manual","","","","1","1","1","1"]
["","Hole protection rubber","","","","2","2","2","2"]
["","Cover","","","","1","1","1","1"]
["","Dew proof material","","","","1","1","1","1"]
["","Remote control wiring","","","","1","1","1","1"]
["","Bracket for installation","","","","1","1","1","1"]
["","Operation manual","","","","1","1","1","1"]
["","Bush","","","","1","1","1","1"]
["","Installation pattern","","","","1","1","1","1"]
["","Insulation for fitting for gas pipe","","","","1","1","1","1"]
["","Insulation for fitting for liquid pipe","","","","1","1","1","1"]
["","Screws","","","","5","5","5","5"]
["","Tie-wraps","","","","5","5","5","5"]
["Stromversorgung","Phase","","","","1~","1~","1~","1~"]
["","Frequenz","","","Hz","50/60","50/60","50/60","50/60"]
["Spannungsversorgung","Spannung","","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Schalldruckpegel","Kühlen","","Schalldruckpegel-=-Kühlen-=-Mittel-=-dB(A)","dB(A)","","47"]
["","Heizen","","Schalldruckpegel-=-Heizen-=-Mittel-=-dB(A)","dB(A)","","44"]
["","","","Nom.","dB(A)","","47"]
["Hinweise","","","","","","(1) - Siehe separate Zeichnung für die elektrischen Daten"]