{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":11,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVQ-C / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FVQ71CVEB / RZQG71L9V1B","FVQ100CVEB / RZQG71L9V1B","FVQ100CVEB / RZQG100L9V1B","FVQ140CVEB / RZQG100L9V1B","FVQ125CVEB / RZQG125L9V1B","FVQ140CVEB / RZQG125L9V1B","FVQ140CVEB / RZQG140L9V1B"]
["Kühlleistung","Nom.","","kW","6.8","","9.5","","12.0","","13.4"]
["Raumkühlen","SEER","","","6.23","6.31","5.61","5.61","5.61","5.61"]
["","Jährlicher Energieverbrauch","","kWh/a","383","378","593","593","749","749"]
["","Leistung","Pdesign","kW","6.80","6.80","9.50","9.50","12.00","12.00"]
["","Energieeffizienzklasse","","","A++","A++","A+","A+","A+","A+"]
["Raumheizen (Durchschnittliches Klima)","Leistung","Pdesign","kW","6.33","6.33","11.30","11.30","11.30","11.30"]
["","SCOP/A","","","4.05","4.05","4.20","4.20","3.87","3.87"]
["","Energieeffizienzklasse","","","A+","A+","A+","A+","A","A"]
["","Jährlicher Energieverbrauch","","kWh/a","2,189","2,189","3,767","3,767","4,088","4,088"]
["Nominale Effizienz","Jährlicher Energieverbrauch","","kWh","1,010","","1,245","","1,870","","2,085"]
["","EER","","","3.37","","3.81","","3.21","","3.21"]
["","COP","","","3.64","","4.14","","3.70","","3.61"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","A","","A","","A"]
["","","Heizen","","A","","A","","A"]
["Heizleistung","Nom.","","kW","7.5","","10.8","","13.5","","15.5"]
["Hinweise","","","","(1) - Jährlicher Energieverbrauch gemäß der Energieetikett-Richtlinie 2002/31/EC","","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU","","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU","","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU"]
["","","","","(2) - SEER und SCOP gemäß EN 14825","","(2) - Nominale Effizienz: Kühlen bei 35 °C/27 °C Nennlast, Heizen bei 7 °C/20 °C Nennlast","","(2) - Nominale Effizienz: Kühlen bei 35 °C/27 °C Nennlast, Heizen bei 7 °C/20 °C Nennlast","","(2) - Nominale Effizienz: Kühlen bei 35 °C/27 °C Nennlast, Heizen bei 7 °C/20 °C Nennlast"]