{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":8,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVQ-C"]
[]
[]
[]
[]
["","","","","FVQ71CVEB","FVQ100CVEB","FVQ125CVEB","FVQ140CVEB"]
["Schalldruckpegel","Heizen","Hoch","dB(A)","43","50","51","53"]
["","","Nom.","dB(A)","41","47","48","51"]
["","","Niedrig","dB(A)","38","44","46","48"]
["","Kühlung","Niedrig","dB(A)","38","44","46","48"]
["","","Hoch","dB(A)","43","50","51","53"]
["","","Nom.","dB(A)","41","47","48","51"]
["Standardzubehör","Bedienungsanleitung","","","Bedienungsanleitung","Bedienungsanleitung","Bedienungsanleitung","Bedienungsanleitung"]
["","Installationsanleitung","","","Installationsanleitung","Installationsanleitung","Installationsanleitung","Installationsanleitung"]
["","Halterung für Installation","","","Halterung für Installation","Halterung für Installation","Halterung für Installation","Halterung für Installation"]
["","Bohrungsschutzgummi","","","Bohrungsschutzgummi","Bohrungsschutzgummi","Bohrungsschutzgummi","Bohrungsschutzgummi"]
["","Buchse","","","Buchse","Buchse","Buchse","Buchse"]
["","Isolierung für die Armatur","","","Isolierung für die Armatur","Isolierung für die Armatur","Isolierung für die Armatur","Isolierung für die Armatur"]
["","Abdeckung","","","Abdeckung","Abdeckung","Abdeckung","Abdeckung"]
["","Klemmen","","","Klemmen","Klemmen","Klemmen","Klemmen"]
["","Schrauben","","","Schrauben","Schrauben","Schrauben","Schrauben"]
["","Installationsmuster","","","Installationsmuster","Installationsmuster","Installationsmuster","Installationsmuster"]
["","Tausicheres Material","","","Tausicheres Material","Tausicheres Material","Tausicheres Material","Tausicheres Material"]
["","Verdrahtung der Fernbedienung","","","Verdrahtung der Fernbedienung","Verdrahtung der Fernbedienung","Verdrahtung der Fernbedienung","Verdrahtung der Fernbedienung"]
["Regelungssysteme","Wired remote control","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["Rohrleitungsanschlüsse","Flüssigkeit","AD","mm","9.52","9.52","9.52","9.52"]
["","Gas","AD","mm","15.9","15.9","15.9","15.9"]
["","Ableitung","","","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26"]
["Leistungsaufnahme","Kühlung","Nom.","kW","0.117","0.238","0.238","0.276"]
["","Heizen","Nom.","kW","0.117","0.238","0.238","0.276"]
["Schallleistungspegel","Kühlung","","dB(A)","55","62","63","65"]
["","Heizen","","dB(A)","55","62","63","65"]
["Abmessungen","Maßeinheit","Breite","mm","600","600","600","600"]
["","","Tiefe","mm","270","350","350","350"]
["","","Höhe","mm","1,850","1,850","1,850","1,850"]
["Gehäuse","Farbe","","","Reinweiß","Reinweiß","Reinweiß","Reinweiß"]
["Gewicht","Maßeinheit","","kg","39","47","47","47"]
["Power supply","Phase","","","1~","1~","1~","1~"]
["","Frequenz","","Hz","50/60","50/60","50/60","50/60"]
["","Spannung","","V","220-240/220","220-240/220","220-240/220","220-240/220"]