{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":8,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXG-K"]
[]
[]
[]
[]
["","","","","","FVXG25K2V1B","FVXG35K2V1B","FVXG50K2V1B"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","0.019, 0.019, 0.019","0.021 (1) (2) (3), 0.021 (1) (2) (3), 0.021 (1) (2) (3)","0.032, 0.032, 0.032"]
["","Heizen","","Nom.","kW","0.022, 0.022, 0.022","0.024 (2) (1) (3), 0.024 (2) (1) (3), 0.024 (2) (1) (3)","0.035, 0.035, 0.035"]
["Gehäuse","Farbe","","","","Reinweiß (6.5Y 9.5/0.5)","Reinweiß (6.5Y 9.5/0.5)","Reinweiß (6.5Y 9.5/0.5)"]
["Abmessungen","Maßeinheit","","Höhe","mm","600","600","600"]
["","","","Breite","mm","950","950","950"]
["","","","Tiefe","mm","215","215","215"]
["Gewicht","Maßeinheit","","","kg","22.0","22.0","22.0"]
["Ventilator","Luftstromvolumen","Kühlung","Hoch","m³/min","8.9","9.1","10.6"]
["","","Kühlen","Mittel","m³/min","7.0","7.2","8.9"]
["","","","Niedrig","m³/min","5.3","5.3","7.3"]
["","","","Flüsterbetrieb","m³/min","4.5","4.5","6.0"]
["","","Heizen","Hoch","m³/min","9.9","10.2","12.2"]
["","","","Mittel","m³/min","7.8","8.0","10.0"]
["","","","Niedrig","m³/min","5.7","5.8","7.8"]
["","","","Flüsterbetrieb","m³/min","4.7","5.0","6.8"]
["Schallleistungspegel","Kühlung","","","dBA","54","55","56"]
["","Heizen","","","dBA","55","56","58"]
["Schalldruckpegel","Kühlung","","Hoch","dBA","38","39","44"]
["","Kühlen","","Mittel","dBA","32","33","40"]
["","","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dBA","26","27","36"]
["","","","Flüsterbetrieb","dBA","23","24","32"]
["","Heizen","","Hoch","dBA","39","40","46"]
["","","","Mittel","dBA","32","33","40"]
["","","","Niedrig","dBA","26","27","34"]
["","","","Flüsterbetrieb","dBA","22","23","30"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","6.35","6.35","6.35"]
["","Gas","","AD","mm","9.50","9.50","12.7"]
["","Ableitung","","","","18","18","18"]
["Regelungssysteme","Infrarot-Fernbedienung","","","","ARC466A2","ARC466A2","ARC466A2"]
["Standardzubehör","Installation manual","","","","1","1","1"]
["","Wireless remote control","","","","1","1","1"]
["","Installation plate","","","","1","1","1"]
["","Thermal insulation (thermal insulation tube)","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2"]
["","Drain hose","","","","1","1","1"]
["","Remote control holder","","","","1","1","1"]
["Stromversorgung","Bezeichnung","","","","V1","V1","V1"]
["","Phase","","","","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50"]
["Spannungsversorgung","Spannung","","","V","220-240","220-240","220-240"]
["Hinweise","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V"]