{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":7,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXM-A / RXM-R9"]
[]
[]
[]
[]
["","","","","FVXM25A3V1B / RXM25R5V1B9","FVXM35A2V1B / RXM35R5V1B9","FVXM35A3V1B / RXM35R5V1B9"]
["Kühlleistung","Min.","","kW","1.30"]
["","Nom.","","kW","2.40"]
["","Max.","","kW","3.50"]
["Heizleistung","Min.","","kW","1.30"]
["","Nom.","","kW","3.40"]
["","Max.","","kW","4.70"]
["Nominale Effizienz","EER","","","4.47"]
["","COP","","","4.55"]
["","Jährlicher Energieverbrauch","","kWh","268"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","A"]
["","","Heizen","","A"]
["Raumkühlen","Energieeffizienzklasse","","","A+++"]
["","Leistung","Pdesign","kW","2.40"]
["","SEER","","","8.55"]
["","Jährlicher Energieverbrauch","","kWh/a","98"]
["Raumheizen (Durchschnittliches Klima)","Energieeffizienzklasse","","","A++"]
["","Leistung","Pdesign","kW","2.30"]
["","SCOP/A","","","4.65"]
["","Raumheizen (Durchschnittliches Klima)-=-Heizleistung Pdh bei -10°-=-kW","","kW","2.03"]
["","Jährlicher Energieverbrauch","","kWh/a","693"]
["Kühlleistung","Min.","","kW","","1.40","1.40"]
["","Max.","","kW","","4.00","4.00"]
["","Nom.","","kW","","3.40","3.40"]
["Nominale Effizienz","Jährlicher Energieverbrauch","","kWh","","424","424"]
["","EER","","","","4.01","4.01"]
["","COP","","","","3.90","3.90"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","","A","A"]
["","","Heizen","","","A","A"]
["Heizleistung","Nom.","","kW","","4.50","4.50"]
["","Min.","","kW","","1.40","1.40"]
["","Max.","","kW","","5.80","5.80"]
["Hinweise","","","","","(1) - Nennkühlleistungen basieren auf: Innentemperatur: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m.","(1) - Nennkühlleistungen basieren auf: Innentemperatur: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m."]
["","","","","","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m.","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m."]
["","","","","","(3) - Siehe separate Zeichnung für den Betriebsbereich","(3) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","","(4) - Siehe separate Zeichnung für die elektrischen Daten","(4) - Siehe separate Zeichnung für die elektrischen Daten"]