{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":8,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXM-A / RXTP-N8"]
[]
[]
[]
[]
["","","","","FVXM25A2V1B / RXTP25N2V1B8","FVXM25A3V1B / RXTP25N2V1B8","FVXM35A2V1B / RXTP35N2V1B8","FVXM35A3V1B / RXTP35N2V1B8"]
["Kühlleistung","Min.","","kW","1.40","","1.40"]
["","Max.","","kW","4.20","","4.30"]
["","Nom.","","kW","2.50","","3.50"]
["Nominale Effizienz","Jährlicher Energieverbrauch","","kWh","328","","510"]
["","EER","","","3.81","","3.43"]
["","COP","","","3.86","","3.54"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","A","","A"]
["","","Heizen","","A","","B"]
["Heizleistung","Nom.","","kW","3.20","","4.00"]
["","Min.","","kW","1.20","","1.20"]
["","Max.","","kW","5.70","","6.20"]
["Hinweise","","","","(1) - Nennkühlleistungen basieren auf: Innentemperatur: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m.","","(1) - Nennkühlleistungen basieren auf: Innentemperatur: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m."]
["","","","","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m.","","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m."]
["","","","","(3) - Siehe separate Zeichnung für die elektrischen Daten","","(3) - Siehe separate Zeichnung für die elektrischen Daten"]
["","","","","(4) - Siehe separate Zeichnung für den Betriebsbereich","","(4) - Siehe separate Zeichnung für den Betriebsbereich"]
["Kühlleistung","Min.","","kW","","1.00","","1.10"]
["","Nom.","","kW","","2.50","","3.50"]
["","Max.","","kW","","4.20","","4.30"]
["Heizleistung","Min.","","kW","","1.00","","1.10"]
["","Nom.","","kW","","3.20","","4.00"]
["","Max.","","kW","","5.70","","6.20"]
["Nominale Effizienz","EER","","","","3.81","","3.43"]
["","COP","","","","3.86","","3.54"]
["","Jährlicher Energieverbrauch","","kWh","","328","","510"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","","A","","A"]
["","","Heizen","","","A","","B"]
["Raumkühlen","Energieeffizienzklasse","","","","A++","","A++"]
["","Leistung","Pdesign","kW","","2.50","","3.50"]
["","SEER","","","","6.50","","6.10"]
["","Jährlicher Energieverbrauch","","kWh/a","","135","","201"]
["Raumheizen (Durchschnittliches Klima)","Energieeffizienzklasse","","","","A++","","A++"]
["","Leistung","Pdesign","kW","","2.50","","3.00"]
["","SCOP/A","","","","4.70","","4.60"]
["","Raumheizen (Durchschnittliches Klima)-=-Heizleistung Pdh bei -10°-=-kW","","kW","","2.50","","3.00"]
["","Jährlicher Energieverbrauch","","kWh/a","","744","","913"]