{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXM-B / RXM-R9"]
[]
[]
[]
[]
["","","","","FVXM25B2V1B / RXM25R5V1B9","FVXM35B2V1B / RXM35R5V1B9"]
["Kühlleistung","Min.","","kW","1.3","1.4"]
["","Nom.","","kW","2.4","3.4"]
["","Max.","","kW","3.5","4"]
["Heizleistung","Min.","","kW","1.3","1.4"]
["","Nom.","","kW","3.4","4.5"]
["","Max.","","kW","4.7","5.8"]
["Nominale Effizienz","EER","","","4.47","4.01"]
["","COP","","","4.55","3.9"]
["","Jährlicher Energieverbrauch","","kWh","268","424"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","A","A"]
["","","Heizen","","A","A"]
["Raumkühlen","Energieeffizienzklasse","","","A+++","A++"]
["","Leistung","Pdesign","kW","2.4","3.4"]
["","SEER","","","8.55","8.11"]
["","Jährlicher Energieverbrauch","","kWh/a","98","147"]
["Raumheizen (Durchschnittliches Klima)","Energieeffizienzklasse","","","A++","A++"]
["","Leistung","Pdesign","kW","2.3","2.8"]
["","SCOP/A","","","4.65","4.63"]
["","Raumheizen (Durchschnittliches Klima)-=-Heizleistung Pdh bei -10°-=-kW","","kW","2.03","2.34"]
["","Jährlicher Energieverbrauch","","kWh/a","693","847"]
["Hinweise","","","","(1) - Nennkühlleistungen basieren auf: Innentemp.: 27°CTK, 19°CFK; Außentemperatur: 35°CTK; äquivalente Länge Kältemittelleitung: 5m; Niveauunterschied: 0m.","(1) - Nennkühlleistungen basieren auf: Innentemp.: 27°CTK, 19°CFK; Außentemperatur: 35°CTK; äquivalente Länge Kältemittelleitung: 5m; Niveauunterschied: 0m."]
["","","","","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5m; Niveauunterschied: 0 m.","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5m; Niveauunterschied: 0 m."]
["","","","","(3) - Siehe separate Zeichnung für den Betriebsbereich","(3) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","(4) - Siehe separate Zeichnung für die elektrischen Daten","(4) - Siehe separate Zeichnung für die elektrischen Daten"]