{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":6,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXTM-B"]
[]
[]
[]
[]
["","","","","","FVXTM30B2V1B"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","0.02"]
["","Heizen","","Nom.","kW","0.03"]
["Gehäuse","Farbe","","","","Weiß"]
["Abmessungen","Maßeinheit","","Höhe","mm","600"]
["","","","Breite","mm","750"]
["","","","Tiefe","mm","238"]
["Gewicht","Maßeinheit","","","kg","17"]
["Ventilator","Luftstromvolumen","Kühlung","Hoch","m³/min","9"]
["","","Kühlen","Mittel","m³/min","6.7"]
["","","","Niedrig","m³/min","4.8"]
["","","","Flüsterbetrieb","m³/min","4"]
["","","Heizen","Hoch","m³/min","9.4"]
["","","","Mittel","m³/min","6.8"]
["","","","Niedrig","m³/min","5.3"]
["","","","Flüsterbetrieb","m³/min","4"]
["Schallleistungspegel","Kühlung","","","dB(A)","53"]
["","Heizen","","","dB(A)","53"]
["Schalldruckpegel","Kühlung","","Hoch","dB(A)","39"]
["","Kühlen","","Mittel","dB(A)","32"]
["","","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dB(A)","25"]
["","","","Flüsterbetrieb","dB(A)","20"]
["","Heizen","","Hoch","dB(A)","39"]
["","","","Mittel","dB(A)","32"]
["","","","Niedrig","dB(A)","25"]
["","","","Flüsterbetrieb","dB(A)","19"]
["Kältemittel","GWP","","","","675"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","6.35"]
["","Gas","","AD","mm","9.5"]
["","Ableitung","","","","VP20 (I.D. 20/O.D. 26)"]
["Regelungssysteme","Infrarot-Fernbedienung","","","","ARC466A90"]
["","Verkabelte Fernbedienung","","","","BRC073A1"]
["Standardzubehör","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","2"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","1"]
["Stromversorgung","Bezeichnung","","","","V1"]
["","Phase","","","","1~"]
["","Frequenz","","","Hz","50"]
["Spannungsversorgung","Spannung","","","V","220-240"]
["Hinweise","","","","","(1) - Kühlen: Innentemperatur: 27°C TK, 19°C FK, Außentemp. 35°C TK, 24°C FK; äquivalente Leitungslänge: 5 m"]
["","","","","","(2) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m"]
["","","","","","(3) - Siehe separate Zeichnung für die elektrischen Daten"]