{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":62,"n_cols":14,"rows_kept":62,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXFA-A"]
[]
[]
[]
[]
["","","","","","FXFA20A2VEB","FXFA25A2VEB","FXFA32A2VEB","FXFA40A2VEB","FXFA50A2VEB","FXFA63A2VEB","FXFA80A2VEB","FXFA100A2VEB","FXFA125A2VEB"]
["Kühlleistung","Gesamtleistung","","Bei Ventilatordrehzahl „Hoch“","kW","2.2","2.8","3.6","4.5","5.6","7.1","9.0","11.2","14.0"]
["Heizleistung","Gesamtleistung","","Bei Ventilatordrehzahl „Hoch“","kW","2.5","3.2","4.0","5.0","6.3","8.0","10.0","12.5","16.0"]
["Leistungsaufnahme&nbsp;– 50&nbsp;Hz","Leistungsaufnahme&nbsp;– 50&nbsp;Hz-=-Kühlen","","Leistungsaufnahme&nbsp;– 50&nbsp;Hz-=-Kühlen-=-Bei Ventilatordrehzahl „Hoch“-=-kW","kW","0.017 (1)","0.017 (1)","0.017 (1)","0.018 (1)","0.023 (1)","0.028 (1)","0.045 (1)","0.078 (1)","0.103 (1)"]
["","Leistungsaufnahme&nbsp;– 50&nbsp;Hz-=-Heizen","","Leistungsaufnahme&nbsp;– 50&nbsp;Hz-=-Heizen-=-Bei Ventilatordrehzahl „Hoch“-=-kW","kW","0.017 (1)","0.017 (1)","0.017 (1)","0.018 (1)","0.023 (1)","0.028 (1)","0.045 (1)","0.078 (1)","0.103 (1)"]
["Abmessungen","Maßeinheit","","Höhe","mm","204","204","204","204","204","204","246","246","288"]
["","","","Breite","mm","840","840","840","840","840","840","840","840","840"]
["","","","Tiefe","mm","840","840","840","840","840","840","840","840","840"]
["Gewicht","Maßeinheit","","","kg","18","18","18","19","21","21","24","24","26"]
["Gehäuse","Material","","","","Galvanisiertes Stahlblech_","Galvanisiertes Stahlblech_","Galvanisiertes Stahlblech_","Galvanisiertes Stahlblech_","Galvanisiertes Stahlblech_","Galvanisiertes Stahlblech_","Galvanisiertes Stahlblech_","Galvanisiertes Stahlblech_","Galvanisiertes Stahlblech_"]
["Ventilator","Ventilator-=-Luftvolumenstrom&nbsp;– 50&nbsp;Hz","Ventilator-=-Luftvolumenstrom&nbsp;– 50&nbsp;Hz-=-Kühlen","Ventilator-=-Luftvolumenstrom&nbsp;– 50&nbsp;Hz-=-Kühlen-=-Bei Ventilatordrehzahl „Hoch“-=-m³/min","m³/min","12.8","12.8","12.8","14.8","15.1","16.6","23.3","28.8","33.0"]
["","","","Ventilator-=-Luftvolumenstrom&nbsp;– 50&nbsp;Hz-=-Kühlen-=-Bei Ventilatordrehzahl „Niedrig“-=-m³/min","m³/min","8.9","8.9","8.9","10.4","10.7","10.7","13.8","13.8","20.6"]
["Kältemittel","Typ","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","GWP","","","","675","675","675","675","675","675","675","675","675"]
["Schallleistungspegel","Kühlen","","Bei Ventilatordrehzahl „Hoch“","dB(A)","49.0","49.0","49.0","51.0","51.0","53.0","55.0","60.0","61.0"]
["Schalldruckpegel","Kühlen","","Bei Ventilatordrehzahl „Hoch“","dB(A)","31.0","31.0","31.0","33.0","33.0","35.0","38.0","43.0","45.0"]
["","","","Bei Ventilatordrehzahl „Mittel“","dB(A)","29.0","29.0","29.0","31.0","31.0","33.0","34.0","37.0","41.0"]
["","","","Bei Ventilatordrehzahl „Niedrig“","dB(A)","28.0","28.0","28.0","29.0","29.0","30.0","30.0","30.0","36.0"]
["","Heizen","","Bei Ventilatordrehzahl „Hoch“","dB(A)","31.0","31.0","31.0","33.0","33.0","35.0","38.0","43.0","45.0"]
["","","","Bei Ventilatordrehzahl „Mittel“","dB(A)","29.0","29.0","29.0","31.0","31.0","33.0","34.0","37.0","41.0"]
["","","","Bei Ventilatordrehzahl „Niedrig“","dB(A)","28.0","28.0","28.0","29.0","29.0","30.0","30.0","30.0","36.0"]
["Rohrleitungsanschlüsse","Flüssigkeit","","Typ","","Bördelverbindung","Bördelverbindung","Bördelverbindung","Bördelverbindung","Bördelverbindung","Bördelverbindung","Bördelverbindung","Bördelverbindung","Bördelverbindung"]
["","","","AD","mm","6","6","6","6","6","6","6","10","10"]
["","Gas","","Typ","","Bördelverbindung","Bördelverbindung","Bördelverbindung","Bördelverbindung","Bördelverbindung","Bördelverbindung","Bördelverbindung","Bördelverbindung","Bördelverbindung"]
["","","","AD","mm","9.52","9.52","9.52","12.7","12.7","12.7","12.7","15.9","15.9"]
["","Ableitung","","","","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)"]
["Geräteblende","Modell","","","","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B"]
["","Abmessungen","","Höhe","mm","65","65","65","65","65","65","65","65","65"]
["","","","Breite","mm","950","950","950","950","950","950","950","950","950"]
["","","","Tiefe","mm","950","950","950","950","950","950","950","950","950"]
["","Gewicht","","","kg","5.5","5.5","5.5","5.5","5.5","5.5","5.5","5.5","5.5"]
["Geräteblende 2","Modell","","","","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B"]
["","Abmessungen","","Höhe","mm","148","148","148","148","148","148","148","148","148"]
["","","","Breite","mm","950","950","950","950","950","950","950","950","950"]
["","","","Tiefe","mm","950","950","950","950","950","950","950","950","950"]
["","Gewicht","","","kg","10.3","10.3","10.3","10.3","10.3","10.3","10.3","10.3","10.3"]
["Geräteblende 3","Modell","","","","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB"]
["","Abmessungen","","Höhe","mm","106","106","106","106","106","106","106","106","106"]
["","","","Breite","mm","950","950","950","950","950","950","950","950","950"]
["","","","Tiefe","mm","950","950","950","950","950","950","950","950","950"]
["","Gewicht","","","kg","6.5","6.5","6.5","6.5","6.5","6.5","6.5","6.5","6.5"]
["Luftfilter","Typ","","","","Kunststoffnetz","Kunststoffnetz","Kunststoffnetz","Kunststoffnetz","Kunststoffnetz","Kunststoffnetz","Kunststoffnetz","Kunststoffnetz","Kunststoffnetz"]
["Standardzubehör","Washer for hanger bracket","","","","8","8","8","8","8","8","8","8","8"]
["","Wire clamp material","","","","7","7","7","7","7","7","7","7","7"]
["","Clamp for drain hose","","","","1","1","1","1","1","1","1","1","1"]
["","Clamps","","","","1","1","1","1","1","1","1","1","1"]
["","Drain hose","","","","1","1","1","1","1","1","1","1","1"]
["","Installation and operation manual","","","","1","1","1","1","1","1","1","1","1"]
["","Installation guide","","","","1","1","1","1","1","1","1","1","1"]
["","Insulation for fitting","","","","2","2","2","2","2","2","2","2","2"]
["","Screws","","","","4","4","4","4","4","4","4","4","4"]
["","Sealing pads","","","","1","1","1","1","1","1","1","1","1"]
["Stromversorgung","Phase","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Frequenz","","","Hz","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60"]
["Spannungsversorgung","Spannung","","","V","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220"]
["Stromstärke&nbsp;– 50&nbsp;Hz","Stromstärke&nbsp;– 50&nbsp;Hz-=-Max. Amperezahl für Sicherung (MFA)-=-A","","","A","6","6","6","6","6","6","6","6","6"]
["Hinweise","","","","","(1) - Werte gelten für Werkeinstellung.","(1) - Werte gelten für Werkeinstellung.","(1) - Werte gelten für Werkeinstellung.","(1) - Werte gelten für Werkeinstellung.","(1) - Werte gelten für Werkeinstellung.","(1) - Werte gelten für Werkeinstellung.","(1) - Werte gelten für Werkeinstellung.","(1) - Werte gelten für Werkeinstellung.","(1) - Werte gelten für Werkeinstellung."]