{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":102,"n_cols":12,"rows_kept":102,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXMA-A"]
[]
[]
[]
[]
["","","","","","FXMA50A5VEB","FXMA63A5VEB","FXMA80A5VEB","FXMA100A5VEB","FXMA125A5VEB","FXMA200AXVMB","FXMA250AXVMB"]
["Schalldruckpegel","Heizen","","Bei Ventilatordrehzahl „Hoch“","dB(A)","","","","","","48.0"]
["","","","Bei Ventilatordrehzahl „Niedrig“","dB(A)","","","","","","45.0"]
["","","","Bei Ventilatordrehzahl „Mittel“","dB(A)","","","","","","46.5"]
["","Kühlung","","Bei Ventilatordrehzahl „Niedrig“","dB(A)","","","","","","45.0"]
["","","","Bei Ventilatordrehzahl „Hoch“","dB(A)","","","","","","48.0"]
["","","","Bei Ventilatordrehzahl „Mittel“","dB(A)","","","","","","46.5"]
["Standardzubehör","Installations- und Bedienungsanleitung","","","","","","","","","1"]
["","Material Kabelklemme","","","","","","","","","1"]
["","Federscheibe","","","","","","","","","2"]
["","Sechskantschraube","","","","","","","","","2"]
["","Unterlegscheibe","","","","","","","","","8"]
["","Sechskantschraube mit Unterlegscheibe","","","","","","","","","49"]
["","Gasanschlussleitung","","","","","","","","","1"]
["","Allgemeine Schutzmaßnahmen","","","","","","","","","1"]
["Kältemittel","GWP","","","","","","","","","675"]
["","Typ","","","","","","","","","R-32"]
["Leistungsaufnahme - 50Hz","Kühlung","","Bei Ventilatordrehzahl „Hoch“","kW","","","","","","0.54"]
["","Heizen","","Bei Ventilatordrehzahl „Hoch“","kW","","","","","","0.54"]
["Kühlleistung","Gesamtleistung","","Bei Ventilatordrehzahl „Hoch“","kW","","","","","","22.4"]
["","Nom.","","","kW","","","","","","22.4"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","","","","","","9.5"]
["","","","Typ","","","","","","","Bördelverbindung"]
["","Gas","","AD","mm","","","","","","19.1"]
["","","","Typ","","","","","","","Flansch"]
["","Ableitung","","","","","","","","","BSP1"]
["Sound power level","Kühlung","","Bei Ventilatordrehzahl „Hoch“","dB(A)","","","","","","75.0"]
["Abmessungen","Maßeinheit","","Breite","mm","","","","","","1,490"]
["","","","Tiefe","mm","","","","","","1,100"]
["","","","Höhe","mm","","","","","","470"]
["Gehäuse","Material","","","","","","","","","Galvanisiertes Stahlblech."]
["","Farbe","","","","","","","","","Unbeschichtet"]
["Gewicht","Maßeinheit","","","kg","","","","","","105"]
["Ventilator","Externer statischer Druck (ESP) – 50Hz","","Hoch","Pa","","","","","","250"]
["","","","Niedrig","Pa","","","","","","50"]
["","Externer statischer Druck (ESP) – 60Hz","","Hoch","Pa","","","","","","250"]
["","","","Niedrig","Pa","","","","","","50"]
["","Luftvolumenstrom - 50 Hz","Kühlung","Bei Ventilatordrehzahl „Hoch“","m³/min","","","","","","62"]
["","","","Bei Ventilatordrehzahl „Niedrig“","m³/min","","","","","","41"]
["Heizleistung","Gesamtleistung","","Bei Ventilatordrehzahl „Hoch“","kW","","","","","","25.0"]
["","Nom.","","","kW","","","","","","25.0"]
["Strom - 50 Hz","Max. Amperezahl für Sicherung (MFA)","","","A","","","","","","6"]
["Power supply","Phase","","","","","","","","","1~"]
["","Bezeichnung","","","","","","","","","VM"]
["","Frequenz","","","Hz","","","","","","50/60"]
["","Spannung","","","V","","","","","","220-240/220-230"]
["Kühlleistung","Gesamtleistung","","Bei Ventilatordrehzahl „Hoch“","kW","5.6","7.1","9.0","11.2","14.0","","28.0"]
["Heizleistung","Gesamtleistung","","Bei Ventilatordrehzahl „Hoch“","kW","6.3","8.0","10.0","12.5","16.0","","31.5"]
["Leistungsaufnahme&nbsp;– 50&nbsp;Hz","Leistungsaufnahme&nbsp;– 50&nbsp;Hz-=-Kühlen","","Leistungsaufnahme&nbsp;– 50&nbsp;Hz-=-Kühlen-=-Bei Ventilatordrehzahl „Hoch“-=-kW","kW","0.125","0.14","0.198","0.191","0.254","","0.65"]
["","Leistungsaufnahme&nbsp;– 50&nbsp;Hz-=-Heizen","","Leistungsaufnahme&nbsp;– 50&nbsp;Hz-=-Heizen-=-Bei Ventilatordrehzahl „Hoch“-=-kW","kW","0.125","0.14","0.198","0.191","0.254","","0.65"]
["Abmessungen","Maßeinheit","","Höhe","mm","300","300","300","300","300","","470"]
["","","","Breite","mm","1,000","1,000","1,000","1,400","1,400","","1,490"]
["","","","Tiefe","mm","700","700","700","700","700","","1,100"]
["Gewicht","Maßeinheit","","","kg","35","35","35","46","46","","115"]
["Gehäuse","Farbe","","","","Unbeschichtet","Unbeschichtet","Unbeschichtet","Unbeschichtet","Unbeschichtet","","Unbeschichtet"]
["","Material","","","","Galvanisiertes Stahlblech_","Galvanisiertes Stahlblech_","Galvanisiertes Stahlblech_","Galvanisiertes Stahlblech_","Galvanisiertes Stahlblech_","","Galvanisiertes Stahlblech_"]
["Erforderliche Zwischendeckenhöhe >-=-mm","mm","","","","350","350","350","350","350"]
["Ventilator","Ventilator-=-Luftvolumenstrom&nbsp;– 50&nbsp;Hz","Ventilator-=-Luftvolumenstrom&nbsp;– 50&nbsp;Hz-=-Kühlen","Ventilator-=-Luftvolumenstrom&nbsp;– 50&nbsp;Hz-=-Kühlen-=-Bei Ventilatordrehzahl „Hoch“-=-m³/min","m³/min","18.0","19.5","25.0","32.0","36.0","","74"]
["","","","Ventilator-=-Luftvolumenstrom&nbsp;– 50&nbsp;Hz-=-Kühlen-=-Bei Ventilatordrehzahl „Niedrig“-=-m³/min","m³/min","15.0","16.0","20.0","23.0","26.0","","52"]
["","Ventilator-=-Externer statischer Druck (ESP) – 50&nbsp;Hz","","Ventilator-=-Externer statischer Druck (ESP) – 50&nbsp;Hz-=-Hoch-=-Pa","Pa","200","200","200","200","200","","250"]
["","Ventilator-=-Externer statischer Druck (ESP) – 60&nbsp;Hz","","Ventilator-=-Externer statischer Druck (ESP) – 60&nbsp;Hz-=-Hoch-=-Pa","Pa","200","200","200","200","200","","250"]
["Kältemittel","Typ","","","","R-32","R-32","R-32","R-32","R-32","","R-32"]
["","GWP","","","","675","675","675","675","675","","675"]
["Schallleistungspegel","Kühlen","","Bei Ventilatordrehzahl „Hoch“","dB(A)","61.0","64.0","67.0","65.0","70.0","","76.0"]
["Schalldruckpegel","Kühlen","","Bei Ventilatordrehzahl „Hoch“","dB(A)","41.0","42.0","43.0","43.0","44.0","","48.0"]
["","","","Bei Ventilatordrehzahl „Mittel“","dB(A)","39.0","40.0","41.0","41.0","42.0","","46.5"]
["","","","Bei Ventilatordrehzahl „Niedrig“","dB(A)","37.0","38.0","39.0","39.0","40.0","","45.0"]
["","Heizen","","Bei Ventilatordrehzahl „Hoch“","dB(A)","41.0","42.0","43.0","43.0","44.0","","48.0"]
["","","","Bei Ventilatordrehzahl „Mittel“","dB(A)","39.0","40.0","41.0","41.0","42.0","","46.5"]
["","","","Bei Ventilatordrehzahl „Niedrig“","dB(A)","37.0","38.0","39.0","39.0","40.0","","45.0"]
["Rohrleitungsanschlüsse","Flüssigkeit","","Typ","","Bördelverbindung","Bördelverbindung","Bördelverbindung","Bördelverbindung","Bördelverbindung","","Bördelverbindung"]
["","","","AD","mm","6.35","6.35","6.35","9.52","9.52","","9.5"]
["","Gas","","Typ","","Bördelverbindung","Bördelverbindung","Bördelverbindung","Bördelverbindung","Bördelverbindung","","Flansch"]
["","","","AD","mm","12.7","12.7","12.7","15.9","15.9","","19.1"]
["","Ableitung","","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","","BSP1"]
["Luftfilter","Typ","","","","Kunststoffnetz","Kunststoffnetz","Kunststoffnetz","Kunststoffnetz","Kunststoffnetz"]
["Standardzubehör","Washer for hanger bracket","","","","8","8","8","8","8"]
["","Drain hose","","","","1","1","1","1","1"]
["","Installation and operation manual","","","","1","1","1","1","1","","1"]
["","Insulation for fitting","","","","2","2","2","2","2"]
["","Metal clamp for drain hose","","","","1","1","1","1","1"]
["","Screws","","","","16","16","16","16","16"]
["","Sealing pad","","","","3","3","3","3","3"]
["Stromversorgung","Bezeichnung","","","","VE","VE","VE","VE","VE","","VM"]
["","Phase","","","","1~","1~","1~","1~","1~","","1~"]
["","Frequenz","","","Hz","50/60","50/60","50/60","50/60","50/60","","50/60"]
["Spannungsversorgung","Spannung","","","V","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","","220-240/220-230"]
["Stromstärke&nbsp;– 50&nbsp;Hz","Stromstärke&nbsp;– 50&nbsp;Hz-=-Max. Amperezahl für Sicherung (MFA)-=-A","","","A","6","6","6","6","6","","6"]
["Ventilator","Ventilator-=-Externer statischer Druck (ESP) – 50&nbsp;Hz","","Ventilator-=-Externer statischer Druck (ESP) – 50&nbsp;Hz-=-Niedrig-=-Pa","Pa","","","","","","","50"]
["","Ventilator-=-Externer statischer Druck (ESP) – 60&nbsp;Hz","","Ventilator-=-Externer statischer Druck (ESP) – 60&nbsp;Hz-=-Niedrig-=-Pa","Pa","","","","","","","50"]
["Standardzubehör","General safety precautions","","","","","","","","","","1"]
["","Wire clamp material","","","","","","","","","","1"]
["","Spring washer","","","","","","","","","","2"]
["","Hexagon head screw","","","","","","","","","","2"]
["","Plain washer","","","","","","","","","","8"]
["","Hexagon head screw with washer","","","","","","","","","","49"]
["","Gas connection pipe","","","","","","","","","","1"]