{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":8,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","GCU-PXB1"]
[]
[]
[]
[]
["","","","","","GCU2020PXB1","GCU2040PXB1","GCU4070PXB1"]
["Kälteleistung","Mittlere Temperatur","","kW","kW","3.39","6.50","12.54"]
["Verdichter","Anzahl der Umdrehungen","","","U/min","4,200","4,800","3,600"]
["Gewicht","Maßeinheit","","","kg","151","155","285"]
["Kältemittel","GWP","","","","1"]
["","Typ","","","","R744 (CO2)"]
["Ventilatormotor","Abgabe","","","W","115","115","230"]
["","Antrieb","","","","EC","EC","EC"]
["Wärmetauscher","Typ","","","","Standard: Cu/Al","Standard: Cu/Al","Standard: Cu/Al"]
["Leistungsaufnahme","Mittlere Temperatur","","Nom.","kW","1.81","3.81","7.99"]
["COP","Mittlere Temperatur","","Nom.","","1.87","1.70","1.57"]
["Abmessungen","Gerät","","Breite","mm","574","574","773"]
["","","","Tiefe","mm","1,452","1,452","1,684"]
["","","","Höhe","mm","799","799","1,438"]
["Ventilatormotor 2","Ausgabe","","","W","115","115","230"]
["Gehäuse","Colour","","","","Hellgrau RAL 7035","Hellgrau RAL 7035","Hellgrau RAL 7035"]
["Ventilator","Type","","","","Axial","Axial","Axial"]
["","Luftstromvolumen","Kühlen","Nom.","m³/min","63","63","126"]
["","Anzahl","","","","1","1","2"]
["Power supply","Phase","","","","3~"]
["","Frequenz","","","Hz","50"]
["","Spannung","","","V","400"]