{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":5,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","JEHCCU-CL1"]
[]
[]
[]
[]
["","","","","JEHCCU0135CL1"]
["Gewicht","Maßeinheit","","kg","61"]
["Abmessungen","Maßeinheit","Breite","mm","876"]
["","","Tiefe","mm","430"]
["","","Höhe","mm","606"]
["Gehäuse","Farbe","","","Hellgrau"]
["Ventilator","Typ","","","Axial"]
["Power supply","Phase","","","1~"]
["","Frequenz","","Hz","50"]
["","Spannung","","V","230"]
["Hinweise","","","","(1) - SRG 20°C, Ta=32°C, Te=-35°C"]
["","","","","(2) - Der Schalldruckpegel wird im Abstand von 10 m in einem schalltoten Raum gemessen."]
["","","","","(3) - Funktionsweise ist angewiesen auf fluorierte Treibhausgase"]