{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MC80Z"]
[]
[]
[]
[]
["","","","","","MC80ZVM"]
["Typ","","","","","Luftreiniger"]
["Betrieb","","","","","Truhengerät mit Verkleidung"]
["Gehäuse","Farbe","","","","Front: White, Top/Side: Dark Grey"]
["Abmessungen","Maßeinheit","","Höhe","mm","630"]
["","","","Breite","mm","315"]
["","","","Tiefe","mm","315"]
["Gewicht","Maßeinheit","","","kg","9.8"]
["Geeignete Raumgröße","m² (2)","","","","62, 124"]
["CADR","m³/h","","","","480"]
["Betriebsart Luftreinigung","Leistungsaufnahme","","Turbo","kW","0.080"]
["","","","M","kW","0.016"]
["","","","N","kW","0.011"]
["","","","Flüsterbetrieb","kW","0.009"]
["Schalldruckpegel","Betriebsart Luftreinigung","","Turbo","dB(A)","55"]
["","","","Mittel","dB(A)","34"]
["","","","Niedrig","dB(A)","25"]
["","","","Flüsterbetrieb","dB(A)","19"]
["Ventilator","Luftstromvolumen","Betriebsart Luftreinigung","Turbo","m³/h","480"]
["","","","Mittel","m³/h","210"]
["","","","Niedrig","m³/h","132"]
["","","","Flüsterbetrieb","m³/h","84"]
["Verfahren für Staubsammeln","","","","","Elektrostatischer HEPA-Filter"]
["Geruchsfilterungsverfahren","","","","","Twin Streamer + Desodorierender Katalysator"]
["Standardzubehör","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["Netzkabel","m","","","","2"]
["Stromversorgung","Phase","","","","1~"]
["","Frequenz","","","Hz","50/60"]
["Spannungsversorgung","Spannung","","","V","220-240/220-230"]
["Hinweise","","","","","(1) - Die abdeckbare Raumgröße bezieht sich auf den Betrieb des Geräts mit maximaler Ventilatordrehzahl (HH). Die abdeckbare Raumgröße ist die Raumgröße, aus der eine bestimmte Menge an Staubpartikeln innerhalb von 30 Minuten entfernt werden kann."]
["","","","","","(2) - Umgerechnet in NRCC-Standards aus Testwerten gemäß JEM 1467."]