{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":63,"n_cols":6,"rows_kept":63,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK55W"]
[]
[]
[]
[]
["","","","","","MCK55WVM"]
["Typ","","","","","Luftreiniger mit Befeuchtung"]
["Betrieb","","","","","Truhengerät mit Verkleidung"]
["Gehäuse","Farbe","","","","Weiß"]
["Abmessungen","Maßeinheit","","Höhe","mm","700"]
["","","","Breite","mm","270"]
["","","","Tiefe","mm","270"]
["Gewicht","Maßeinheit","","","kg","9.5"]
["Geeignete Raumgröße","m²","","","","41 (1), 82 (2)"]
["CADR","m³/h","","","","320"]
["Betriebsart Luftreinigung","Leistungsaufnahme","","Turbo","kW","0.056"]
["","","","M","kW","0.017"]
["","","","N","kW","0.010"]
["","","","Flüsterbetrieb","kW","0.007"]
["Betriebsart Befeuchtung","Leistungsaufnahme","","Turbo","kW","0.058"]
["","","","M","kW","0.019"]
["","","","N","kW","0.014"]
["","","","Flüsterbetrieb","kW","0.011"]
["","Füllmenge Wassertank","","","l","2.7"]
["Schalldruckpegel","Betriebsart Luftreinigung","","Turbo","dBA","53.0"]
["","","","Mittel","dBA","39.0"]
["","","","Niedrig","dBA","29.0"]
["","","","Flüsterbetrieb","dBA","19.0"]
["","Betriebsart Befeuchtung","","Schalldruckpegel-=-Betriebsart Befeuchtung-=-Turbo-=-dB(A)","dBA","53.0"]
["","","","Mittel","dBA","39.0"]
["","","","Niedrig","dBA","33.0"]
["","","","Flüsterbetrieb","dBA","25.0"]
["Ventilator","Luftstromvolumen","Betriebsart Luftreinigung","Turbo","m³/h","330"]
["","","","Mittel","m³/h","192"]
["","","","Niedrig","m³/h","120"]
["","","","Flüsterbetrieb","m³/h","54"]
["","","Betriebsart Befeuchtung","Turbo","m³/h","330"]
["","","","Mittel","m³/h","192"]
["","","","Niedrig","m³/h","144"]
["","","","Flüsterbetrieb","m³/h","102"]
["Verfahren für Staubsammeln","","","","","Elektrostatischer HEPA-Filter"]
["Geruchsfilterungsverfahren","","","","","Flash Streamer + Desodorierender Katalysator"]
["Standardzubehör","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["","Caster","","","","4"]
["","Humidifying filter","","","","2"]
["","Remote control holder","","","","1"]
["","Remote control lid","","","","1"]
["Netzkabel","Netzkabel","","","","1.8"]
["Stromversorgung","Phase","","","","1~"]
["","Stromversorgung-=-Frequenz","","Frequenz","","50/60"]
["Spannungsversorgung","Spannungsversorgung-=-Spannung","","Spannung","","220-240/220-230"]
["Betriebsstrom","Betriebsart Luftreinigung","Betriebsstrom-=-Betriebsart Luftreinigung-=-Turbo","Turbo","","0.50"]
["","","Betriebsstrom-=-Betriebsart Luftreinigung-=-Mittel","Mittel","","0.19"]
["","","Betriebsstrom-=-Betriebsart Luftreinigung-=-Niedrig","Niedrig","","0.12"]
["","","Betriebsstrom-=-Betriebsart Luftreinigung-=-Flüsterbetrieb","Flüsterbetrieb","","0.09"]
["","Betriebsart Befeuchtung","Betriebsstrom-=-Betriebsart Befeuchtung-=-Turbo","Turbo","","0.50"]
["","","Betriebsstrom-=-Betriebsart Befeuchtung-=-Mittel","Mittel","","0.20"]
["","","Betriebsstrom-=-Betriebsart Befeuchtung-=-Niedrig","Niedrig","","0.15"]
["","","Betriebsstrom-=-Betriebsart Befeuchtung-=-Flüsterbetrieb","Flüsterbetrieb","","0.13"]
["Hinweise","","","","","(1) - Die anwendbare Raumfläche bezieht sich auf den Betrieb des Geräts mit maximaler Ventilatordrehzahl (HH). Die maximale Raumgröße bezieht sich auf eine Raumgröße, aus der eine bestimmte Menge an Staubpartikeln innerhalb von 30 Minuten entfernt werden kann. (JEM 1467)"]
["","","","","","(2) - Umgerechnet in NRCC-Standards aus Testwerten gemäß JEM 1467."]