{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":59,"n_cols":6,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK70ZW"]
[]
[]
[]
[]
["","","","","","MCK70ZVM-W"]
["Typ","","","","","Luftreiniger mit Befeuchtung"]
["Anwendung","","","","","Truhengerät mit Verkleidung"]
["Gehäuse","Farbe","","","","White (9.9YR/9.4/0.2)"]
["Abmessungen","Maßeinheit","","Höhe","mm","760"]
["","","","Breite","mm","315"]
["","","","Tiefe","mm","315"]
["Gewicht","Maßeinheit","","","kg","12.5"]
["Geeignete Raumgröße","m² (2)","","","","48 (1), 96 (2)"]
["CADR","m³/h","","","","375"]
["Betriebsart Luftreinigung","Leistungsaufnahme","","Turbo","kW","0.082"]
["","","","M","kW","0.020"]
["","","","N","kW","0.011"]
["","","","Flüsterbetrieb","kW","0.010"]
["Betriebsart Befeuchtung","Leistungsaufnahme","","Turbo","kW","0.084"]
["","","","M","kW","0.023"]
["","","","N","kW","0.012"]
["","","","Flüsterbetrieb","kW","0.010"]
["","Füllmenge Wassertank","","","l","3.4"]
["Schalldruckpegel","Betriebsart Luftreinigung","","Turbo","dB(A)","54"]
["","","","Mittel","dB(A)","37"]
["","","","Niedrig","dB(A)","27"]
["","","","Flüsterbetrieb","dB(A)","18"]
["","Betriebsart Befeuchtung","","Turbo","dB(A)","54"]
["","","","Mittel","dB(A)","37"]
["","","","Niedrig","dB(A)","27"]
["","","","Flüsterbetrieb","dB(A)","18"]
["Ventilator","Luftstromvolumen","Betriebsart Luftreinigung","Turbo","m³/h","420"]
["","","","Mittel","m³/h","210"]
["","","","Niedrig","m³/h","132"]
["","","","Flüsterbetrieb","m³/h","84"]
["","","Betriebsart Befeuchtung","Turbo","m³/h","420"]
["","","","Mittel","m³/h","210"]
["","","","Niedrig","m³/h","132"]
["","","","Flüsterbetrieb","m³/h","84"]
["Verfahren für Staubsammeln","","","","","Elektrostatischer HEPA-Filter"]
["Geruchsfilterungsverfahren","","","","","Flash Streamer + Desodorierender Katalysator"]
["Standardzubehör","Elektrostatischer HEPA-Filter","","","","1"]
["","Befeuchtungsfilter","","","","2"]
["","Geruchsbindender Filter","","","","1"]
["","Installations- und Bedienungsanleitung","","","","1"]
["","Rolle","","","","4"]
["Netzkabel","m","","","","2"]
["Power supply","Phase","","","","1~"]
["","Frequenz","","","Hz","50/60"]
["","Spannung","","","V","220-240/220-230"]
["Hinweise","","","","","(1) - Die abdeckbare Raumgröße bezieht sich auf den Betrieb des Geräts mit maximaler Ventilatordrehzahl (HH). Die abdeckbare Raumgröße ist die Raumgröße, aus der eine bestimmte Menge an Staubpartikeln innerhalb von 30 Minuten entfernt werden kann."]
["","","","","","(2) - Umgerechnet in NRCC-Standards aus Testwerten gemäß JEM 1467."]
["","","","","","(3) - Umgerechnet in CADR-Standards aus Testwerten gemäß JEM 1467."]
["","","","","","(4) - Die Befeuchtungsleistung ändert sich mit Temperatur und Luftfeuchte der Raumluft und der Außenluft. Messbedingungen: Raumtemperatur 20°C, Raumluftfeuchte 30 %."]
["","","","","","(5) - Betriebsschallpegel sind Mittelwerte, gemessen in 1 m Entfernung von Vorderseite, linker Seite, rechter Seite und Oberseite des Geräts. (Diese entsprechen den Werten in einem schalltoten Raum.)"]
["","","","","","(6) - Elektrostatischer HEPA-Filter und Befeuchtungsfilter sind in das Gerät integriert."]
["","","","","","(7) - Anforderungen entsprechend JEM1467."]
["","","","","","(8) - „HI“ wird angezeigt, wenn die PM2,5-Konzentration 99 µg/m³ überschreitet."]