{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":7,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","NHY2KOMB-A / EJHA-AV3"]
[]
[]
[]
[]
["","","","","","NHY2KOMB28AA / EJHA04AAV3","NHY2KOMB32AA / EJHA04AAV3"]
["Warmwasserbereitung","Allgemein","","Deklariertes Lastprofil","","XL","XL"]
["","Durchschnittliches Klima","","Energieeffizienzklasse Wasserheizung","","A","A"]
["COP","","","","","4.49 (1)","4.49 (1)"]
["Pumpe","ESP","Heizung","Min.","kPa","25.0 (4)","25.0 (4)"]
["","","","Max.","kPa","45.0 (4)","45.0 (4)"]
["Raumheizen","Wasserauslass 55 °C für durchschnittliches Klima","Allgemein","Seasonal space heating eff. class","","A++","A++"]
["","","","ηs (Saisonale Effizienz Raumheizen)","%","128","128"]
["","","","SCOP","","3.26","3.28"]
["Heizleistung","Nom.","","","kW","3.83 (1)","3.83 (1)"]
["","Max.","","","kW","4.53 (1)","4.53 (1)"]
["Leistungsaufnahme","Heizen","","Max.","kW","1.07 (1)","1.07 (1)"]
["","","","Nom.","kW","0.850 (1)","0.850 (1)"]
["Hinweise","","","","","(1) - Heizen: Wassertemp. Kondensatoraustritt 35°C, Dt 5 K; Umgebungstemp. 7°C Trockenkugel, 6°C Feuchtkugel","(1) - Heizen: Wassertemp. Kondensatoraustritt 35°C, Dt 5 K; Umgebungstemp. 7°C Trockenkugel, 6°C Feuchtkugel"]
["","","","","","(2) - TK/FK 7 °C/6 °C – LWC 35 °C(dT=5 °C), Boiler-Bypass","(2) - TK/FK 7 °C/6 °C – LWC 35 °C(dT=5 °C), Boiler-Bypass"]
["","","","","","(3) - TK/FK 7 °C/6 °C – LWC 45 °C(dT=5 °C), Boiler-Bypass","(3) - TK/FK 7 °C/6 °C – LWC 45 °C(dT=5 °C), Boiler-Bypass"]
["","","","","","(4) - Abhängig von der Länge der bauseitigen Leitung","(4) - Abhängig von der Länge der bauseitigen Leitung"]