{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":7,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","NHY2KOMB-A"]
[]
[]
[]
[]
["","","","","","NHY2KOMB28AA","NHY2KOMB32AA"]
["Gas","Anschluss","","Durchmesser","mm","15","15"]
["","Verbrauch (G20)","","Min.","m³/h","0.74","0.79"]
["","","","Max.","m³/h","3.02","3.39"]
["","Verbrauch (G25)","","Min.","m³/h","0.84","0.89"]
["","","","Max.","m³/h","3.46","3.92"]
["","Verbrauch (G31)","","Min.","m³/h","0.28","0.30"]
["","","","Max.","m³/h","1.15","1.29"]
["","NOx-klasse","","","","6","6"]
["Zentralheizung","Heizaufnahme Qn (Netto-Brennwert)","Nom.","Min.","kW","7.1","7.6"]
["","","","Max.","kW","23.7","27.0"]
["","Heizaufnahme Qn (Brutto-Brennwert)","Nom.","Min.","kW","8.0","8.3"]
["","","","Max.","kW","26.3","30.0"]
["","Zentralheizung-=-Abgabe Pn bei 80/60 °C","","Zentralheizung-=-Abgabe Pn bei 80/60 °C-=-Min.-=-kW","kW","7.1","7.4"]
["","","","Zentralheizung-=-Abgabe Pn bei 80/60 °C-=-Nom.-=-kW","kW","23.1","26.6"]
["","Zentralheizung-=-Abgabe Pnc bei 50/30 °C","","Zentralheizung-=-Abgabe Pnc bei 50/30 °C-=-Min.-=-kW","kW","7.7","8.2"]
["","","","Zentralheizung-=-Abgabe Pnc bei 50/30 °C-=-Nom.-=-kW","kW","25.4","28.9"]
["Trinkwassererwärmung","Heizaufnahme (Netto-Brennwert) Qnw","Nom.","Min.","kW","7.2","7.6"]
["","","","Max.","kW","29.1","32.7"]
["","Heizaufnahme (Brutto-Brennwert) Qnw","Nom.","Min.","kW","7.9","8.4"]
["","","","Max.","kW","32.3","36.2"]
["","Effizienz","","Nom.","%","105","105"]
["Zufuhrluft","Anschluss","","","mm","100","100"]
["","Konzentrisch","","","","Ja","Ja"]
["Rauchgas","Anschluss","","","mm","60","60"]
["Gehäuse","Farbe","","","","Weiß – RAL9010","Weiß – RAL9010"]
["","Material","","","","Vorbeschichtetes Blech","Vorbeschichtetes Blech"]
["Abmessungen","Gerät","Höhe","Gehäuse","mm","650","710"]
["","Maßeinheit","","Breite","mm","450","450"]
["","","","Tiefe","mm","240","240"]
["Gewicht","Gerät","","Voll","kg","33","36"]
["Trinkwassererwärmung","Allgemein","","Deklariertes Lastprofil","","XL","XL"]
["","","","Energieeffizienzklasse Wasserheizung","","A","A"]
["Raumheizen","Allgemein","","Saisonale Effizienzklasse Raumheizen","","A","A"]
["Energieeffizienzbereich","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Hinweise","","","","","(1) - 80/60","(1) - 80/60"]
["","","","","","(2) - Sollwert 60°C","(2) - Sollwert 60°C"]
["","","","","","(3) - Sollwert 40°C","(3) - Sollwert 40°C"]