{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":7,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","NHY2KOMB-A"]
[]
[]
[]
[]
["","","","","","NHY2KOMB28AA","NHY2KOMB32AA"]
["Trinkwassererwärmung","Heizaufnahme (Brutto-Brennwert) Qnw","Nom.","Max.","kW","32.3","36.2"]
["","","","Min.","kW","7.9","8.4"]
["","Heizaufnahme (Netto-Brennwert) Qnw","Nom.","Min.","kW","7.2","7.6"]
["","","","Max.","kW","29.1","32.7"]
["","Effizienz","","Nom.","%","105","105"]
["Zufuhrluft","Konzentrisch","","","","Ja","Ja"]
["Trinkwassererwärmung","Allgemein","","Energieeffizienzklasse Wasserheizung","","A","A"]
["","","","Deklariertes Lastprofil","","XL","XL"]
["Abmessungen","Maßeinheit","Höhe","Gehäuse","mm","650","710"]
["Gehäuse","Material","","","","Vorbeschichtetes Blech","Vorbeschichtetes Blech"]
["","Farbe","","","","Weiß – RAL9010","Weiß – RAL9010"]
["Raumheizen","Allgemein","","Saisonale Effizienzklasse Raumheizen","","A","A"]
["","","","ηs (Saisonale Effizienz Raumheizen)","%","93","93"]
["Zentralheizung","Heizaufnahme Qn (Brutto-Brennwert)","Nom.","Min.","kW","8.0","8.3"]
["","","","Max.","kW","26.3","30.0"]
["","Abgabe Pn bei 80/60°C","","Min.","kW","7.1","7.4"]
["","","","Nom.","kW","23.1","26.6"]
["","Heizaufnahme Qn (Netto-Brennwert)","Nom.","Max.","kW","23.7","27.0"]
["","","","Min.","kW","7.1","7.6"]
["","Abgabe Pnc bei 50/30°C","","Min.","kW","7.7","8.2"]
["","","","Nom.","kW","25.4","28.9"]
["Gas","Anschluss","","Durchmesser","mm","15","15"]
["","Verbrauch (G31)","","Min.","m³/h","0.28","0.30"]
["","","","Max.","m³/h","1.15","1.29"]
["","NOx-klasse","","","","6","6"]
["Hinweise","","","","","(1) - 80/60","(1) - 80/60"]
["","","","","","(2) - Sollwert 60 °C","(2) - Sollwert 60 °C"]
["","","","","","(3) - Sollwert 40 °C","(3) - Sollwert 40 °C"]