{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":8,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXA-A8"]
[]
[]
[]
[]
["","","","","","RXA20A5V1B8","RXA25A5V1B8","RXA35A5V1B8"]
["Abmessungen","Maßeinheit","","Höhe","mm","550","550","550"]
["","","","Breite","mm","840","840","840"]
["","","","Tiefe","mm","350","350","350"]
["Gewicht","Maßeinheit","","","kg","32","32","32"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°C TK","-10","-10","-10"]
["","","","Max.","°C TK","46","46","46"]
["","Heizen","Umgebung","Betriebsbereich-=-Heizen-=-Umgebung-=-Min.-=-°C FK","°C FK","-15","-15","-15"]
["","","","Betriebsbereich-=-Heizen-=-Umgebung-=-Max.-=-°C FK","°C FK","18","18","18"]
["Schalldruckpegel","Kühlung","","Nom.","dB(A)","46.0","46.0","49.0"]
["","Heizen","","Nom.","dB(A)","47.0","47.0","49.0"]
["Kältemittel","Typ","","","","R-32","R-32","R-32"]
["","Füllmenge","","","kg","0.76","0.76","0.76"]
["","Kältemittel-=-Füllmenge-=-tCO2-Äq.","","","tCO2-Äq.","0.52","0.52","0.52"]
["","GWP","","","","675.0","675.0","675.0"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","AG – IG","m","20","20","20"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)"]
["","Niveauunterschied","IG - AG","Max.","m","15.0","15.0","15.0"]
["Standardzubehör","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","General safety precautions","","","","1"]
["","Drain plug","","","","1"]
["Energieeffizienzbereich","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Stromversorgung","Phase","","","","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50"]
["Spannungsversorgung","Spannung","","","V","220-240","220-240","220-240"]
["Hinweise","","","","","(1) - Enthält fluorierte Treibhausgase","(1) - Enthält fluorierte Treibhausgase","(1) - Enthält fluorierte Treibhausgase"]
["","","","","","(2) - Siehe separate Zeichnung für den Betriebsbereich","(2) - Siehe separate Zeichnung für den Betriebsbereich","(2) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","","(3) - Siehe separate Zeichnung für die elektrischen Daten","(3) - Siehe separate Zeichnung für die elektrischen Daten","(3) - Siehe separate Zeichnung für die elektrischen Daten"]
["Standardzubehör","Installationsanleitung","","","","","1","1"]
["","Etikett für Kältemittelfüllmenge","","","","","1","1"]
["","Mehrsprachige Etiketten über fluorierte Treibhausgase","","","","","1","1"]
["","Allgemeine Schutzmaßnahmen","","","","","1","1"]
["","Ablassstopfen","","","","","1","1"]