{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":7,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXA-B8"]
[]
[]
[]
[]
["","","","","","RXA42B5V1B8","RXA50B5V1B8"]
["Abmessungen","Maßeinheit","","Höhe","mm","734","734"]
["","","","Breite","mm","954","954"]
["","","","Tiefe","mm","401","401"]
["Gewicht","Maßeinheit","","","kg","49","49"]
["Verdichter","Typ","","","","Vollhermetischer Swing-Verdichter","Vollhermetischer Swing-Verdichter"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°C Trockenkugel","-10","-10"]
["","","","Max.","°C Trockenkugel","46","46"]
["","Heizen","Umgebung","Min.","°C Feuchtkugel","-15","-15"]
["","","","Max.","°C Feuchtkugel","18","18"]
["Schalldruckpegel","Kühlung","","Schalldruckpegel-=-Kühlung-=-Nom.-=-dBA","dBA","48","48"]
["","Heizen","","Schalldruckpegel-=-Heizen-=-Nom.-=-dBA","dBA","48","48"]
["Kältemittel","Typ","","","","R-32","R-32"]
["","Füllmenge","","","kg","1.1","1.1"]
["","Füllmenge","","","tCO2Eq","0.75","0.75"]
["","GWP","","","","675","675"]
["Rohrleitungsanschlüsse","Leitungslänge","Max.","AG – IG","M","30","30"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","0,02 (für Rohrleitungslängen über 10 m)","0,02 (für Rohrleitungslängen über 10 m)"]
["","Niveauunterschied","IG - AG","Max.","M","20","20"]
["Standardzubehör","Installation manual","","","","1","1"]
["","Refrigerant charge label","","","","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1"]
["","Drain cap","","","","3","3"]
["","Drain plug","","","","1","1"]
["Stromversorgung","Phase","","","","1~","1~"]
["","Frequenz","","","Hz","50","50"]
["Spannungsversorgung","Spannung","","","V","220-240","220-240"]
["Hinweise","","","","","(1) - Siehe separate Zeichnung für den Betriebsbereich","(1) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","","(2) - Siehe separate Zeichnung für die elektrischen Daten","(2) - Siehe separate Zeichnung für die elektrischen Daten"]
["","","","","","(3) - Enthält fluorierte Treibhausgase","(3) - Enthält fluorierte Treibhausgase"]